Australian Capital Territory
Gaming Machine (Peripheral Equipment) Approval 2011 (No 2)
Notifiable instrument NI2011– 7
made under the  
Gaming Machine Act 2004, section 69 (Approval of gaming machines and peripheral equipment)

1	Name of instrument
This instrument is the Gaming Machine (Peripheral Equipment) Approval 2011 (No 2).

2	Commencement 
This instrument commences the day after the date of notification.

3	Approval
I approve the peripheral equipment described in the attached Schedule to this instrument.  

Lesley Maloney
Delegate
ACT Gambling and Racing Commission

12 January 2011

Monitoring System Software Update 	
Manufacturer	IGT (Australia) Pty Ltd	
System Name	IGT Systems Max	
Category 	Subsidiary Equipment	
Specification 	18.SET03	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard V4.18	
System Software Identifier	3.2T	
The IGT Systems Max version 3.2T is approved to operate with the following Cash Redemption Terminal	
System Name	eCash Redemption Terminal	
Specification Number	18.SER01	
Category	Gaming Support Systems	
Submission Standards	NS 9.0 + NSW Appendix (dated 23/03/07)	
Technical Standards	NS 9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2; TITO Technical Standard 4.18	

Controller Firmware	Version 02.00.03.08	
Interface Card Firmware	Version 1.21	
Specific Approval Conditions
1.	Use of the Xtra Credit facility is subject to the requirements of the Gaming Machine Act 2004 and Gambling and Racing Control (Code of Practice) Regulation 2002.
2.	The Xtra Credit functionality is limited to single venue use only.	
Operational Conditions
1.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine. 
2.	The “IGT Systems Max” is approved for use in a local area network (LAN) configuration only.
3.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS).  The UPS must have sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption.  Desirably the system should be equipped with a “Smart” UPS capable of automatically shutting the system down in the case of a power failure.
4.	The system must be configured in such a way that only authorised personnel have access to critical functions and sensitive information contained in the system.	
Application Reference Number	18.A1210/S01	

Updated Jackpot Controller Software 	
System Name	Standard LPJS – Mystical Temple	
Manufacturer	Konami Australia Pty Ltd	
Category	Progressive Controller	
Category Type	Standard Progressive Controller	
Specification 	39.YA002	
Submission Standards
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standards Rev 1.1	
Controller Firmware	Version 09	
Interface Card Firmware	Version 05	
Jackpot Theme	Mystical Temple	
Operational Conditions
The system interface card must be enclosed in a sealed enclosure.	
Application Reference Number	39-A0909/S01