Australian Capital Territory

**Water Resources (Water Available from Areas) Determination 2024**

**Disallowable instrument DI2024—8**

made under the

**Water Resources Act 2007, s 17 (Amounts of water available from areas)**

1. **Name of instrument**

This instrument is the *Water Resources (Water Available from Areas) Determination 2024.*

**2 Commencement**

This instrument commences on the day after its notification day.

**3 Determination of amounts of water available from areas**

I determine the total amount of surface water and ground water available for taking from each ACT water management area in schedule 1.

**4 Revocation**

This instrument revokes the *Water Resources (Water Available from Areas) Determination 2019* (No 2) (DI2019-191).

Shane Rattenbury MLA

Minister for Water, Energy and Emissions Reduction

14 January 2024

**Schedule 1**

(see section 3)

**Water available for taking from whole of ACT water management area (ACT Water Resource Plan Area)**

**Total amount of surface water available for taking from ACT Water Resource Plan (Surface Water) water management area**

Total surface water available for taking (GL per annum) from ACT Water Resource Plan (Surface water) water management area - The ACT’s overall total surface water available for taking is limited and shall be managed so as to not exceed the ACT’s surface water Sustainable Diversion Limit, as detailed in the ACT Water Resource Plan, under the Murray-Darling Basin Plan:

42.7 GL per annum (net take from water courses), plus

11 GL per annum (take by Commercial Plantations), plus

4.64 GL per annum (take by Runoff Dams), minus

4.9 GL per annum shared reduction amount (towards the Basin-wide water recovery target), plus

Net interstate trade volume (trade into ACT minus trade out of ACT).

Note 1. The net take from water courses is calculated based on the gross take from water courses less return flows which include discharges to waterways from sewage treatment plants (the Lower Molonglo Water Quality Control Centre and the Queanbeyan Sewage Treatment Plant). Under the ACT Water Resource Plan it is proposed that increased flows (stormwater runoff) as a result of increased urbanisation (increased impervious areas) since July 2009 are also included as a return flow for calculating net take.

Note 2. In addition to these total amounts of surface water available for taking from the ACT water resource plan area, the total amount of water available for taking from individual sub water management areas is limited and shall be managed such as to not exceed the volumes listed in Table 1.

**Total amount of groundwater available for taking from ACT Water Resource Plan (Groundwater) water management area**

Total groundwater available for taking (GL per annum) from ACT Water Resource Plan (Groundwater) water management area - The ACT’s overall total groundwater available for taking is limited and shall be managed such as to not exceed the ACT’s groundwater Sustainable Diversion Limit, as detailed in the ACT Water Resource Plan, under the Murray-Darling Basin Plan, of 3.16 GL per annum.

Note 3. In addition to these total amounts of groundwater available for taking from the ACT water resource plan area, the total amount of water available for taking from individual sub water management areas is limited and shall be managed such as to not exceed the volumes listed in Table 1.

**Table 1: Water available for taking from each sub water management area**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sub Water Management Area** | **Total ACT controlled surface water plus ground water (ML/yr)** | **ACT environmental allocation (ML/yr)** | **Total surface water available for taking (ML/yr)** | **Total ground water available for taking (ML/yr)** |
| Central Molonglo | 29,747 | 23,319 | 5,743 | 685 |
| Cotter | 106,565 | 22,849 | 81,666 | 2,050 |
| Ginninderra | 21,488 | 19,188 | 2,061 | 239 |
| Googong | 63,215 | 8,030 | 55,185 | 0 |
| Gudgenby | 33,522 | 29,350 | 3,002 | 1,170 |
| Jerrabomberra | 0 | 0 | 0 | 0 |
| Lower Molonglo | 46,124 | 13,886 | 31,941 | 297 |
| Lower Murrumbidgee | 11,497 | 10,239 | 1,069 | 189 |
| Lower Queanbeyan | 0 | 0 | 0 | 0 |
| Naas | 16,476 | 14,149 | 1,472 | 855 |
| Paddys | 34,583 | 30,621 | 3,053 | 909 |
| Tuggeranong | 8,507 | 7,492 | 825 | 190 |
| Upper Molonglo | 2,403 | 2,139 | 240 | 24 |
| Upper Murrumbidgee | 19,833 | 17,418 | 1,775 | 640 |
| **Overall total** | **393,960** | **198,680** | **188,032** | **7,248** |

Note 5: Total ACT controlled water and environmental allocations were derived from the ACT Source Model (Alluvium 2018) and based on the current Environmental Flow Guidelines. 1 GL equals 1000 ML