Australian Capital Territory
Gaming Machine (Peripheral Equipment) Approval 2009 (No 18)
Notifiable instrument NI2009– 557
made under the  
Gaming Machine Act 2004, section 69 (Approval of gaming machines and peripheral equipment)

1	Name of instrument
This instrument is the Gaming Machine (Peripheral Equipment) Approval 2009 (No 18).

2	Commencement 
This instrument commences the day after the date of notification.

3	Approval
I approve the gaming machine(s) and/or peripheral equipment described in the attached Schedule to this instrument.  

4	Revocation
This instrument revokes notifiable instrument NI2009-73 dated 
25 February 2009 and notified under the Legislation Register on 
2 March 2009.

Lesley Maloney
Delegate
ACT Gambling and Racing Commission
2 November 2009

SYSTEM/DEVICE NAME	Standard/Hyperlink Link Progressive Jackpot System^+	
MANUFACTURER	Aristocrat Technologies Australia Pty Ltd	
CATEGORY	PC	
SPECIFICATION OR
SERIAL NUMBER	01-YA001 (SLPJS)
01-SES00 (ATA Graphics Server)
01-SES01 (Thin Client ATA Graphics Server)	
APPLICATION REFERENCE NUMBER	01-A1039/S01, 01-A1040/S01, /S02	
TECHNICAL STANDARDS	NSW Jackpot TS Rev 1.1
NSW CPTS 2.2	
SUBMISSION STANDARDS	NS 9.0 + NSW Appendix (dated 23/03/07)	
^Operational Conditions:  
1.	There should be at lease one venue overhead display connected to the ATA Graphics Server so as to display pool values, the GMID/House Number of the winning gaming machine, jackpot win amounts and the G-Line message.
2.	When the above-mentioned Standard/Hyperlink LPJS is set up in a ‘Dollar Link’ configuration, then separate ATA Graphic Servers must drive the top box in-machine displays, so as to provide appropriate game theme content (The Bull Fighter & Dollar Eagle).
•	In such cases, any ATA Graphics Server that does not connect to a venue overhead display, must ensure that a VGA Loop Back Adaptor terminates the video signal on the primary port of the two-way splitter that connects to the ATA Graphics Server output port, so as to ensure that the top box in-machine display receives game themed content.
3.	The ATA Graphics Server must be connected to the above-mentioned Standard/Hyperlink LPJS.
4.	The ATA Graphics Server active external I/O ports must be housed in a security cage fitted with a security seal to prevent connection or removal of data cables.
+Note:	Refer to NSW approval for list of approved hyperlink games approved/authorised to operate with the above-mentioned Standard/Hyperlink LPJS.

SYSTEM/DEVICE NAME	IGT Systems Max^*	
MANUFACTURER	IGT (Australia) Pty Ltd	
CATEGORY	SE	
SPECIFICATION OR
SERIAL NUMBER	18-SET03	
APPLICATION REFERENCE NUMBER	18-A1165/S01	
TECHNICAL STANDARDS	NSW CPTS 2.2
TITO Technical Standard V4.18	
SUBMISSION STANDARDS	NS 9.0 + NSW Appendix (dated 23/03/07)	
^Operational Conditions:  
1.	The system VIP functionality must be disabled during installation.
2.	The system must be fitted with a compliance plate.
3.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine.
4.	The system is approved for use in a local area network (LAN) configuration only.
5.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS).  The UPS must have sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption.  Desirably the system should be equipped wit a “Smart” UPS capable of automatically shutting the system down in the case of a power failure.
*Note:	The “Ticket In” and “Cashless” facilities are not approved in the ACT.

SYSTEM/DEVICE NAME	IGT Systems Max*	
MANUFACTURER	IGT (Australia) Pty Ltd	
CATEGORY	SE	
SPECIFICATION OR
SERIAL NUMBER	18-SET03	
APPLICATION REFERENCE NUMBER	18-A1170/S01	
TECHNICAL STANDARDS	NS 9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard V4.18	
SUBMISSION STANDARDS	NS 9.0 + NSW Appendix (dated 23/03/07)	
^Operational Conditions:  
1.	The system VIP functionality must be disabled during installation.
2.	The system must be fitted with a compliance plate.
3.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine.
4.	The system is approved for use in a local area network (LAN) configuration only.
5.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS).  The UPS must have sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption.  Desirably the system should be equipped wit a “Smart” UPS capable of automatically shutting the system down in the case of a power failure.
*Note: 	The “Ticket In” and “Cashless” facilities are not approved in the ACT.

SYSTEM/DEVICE NAME	IGT Systems Max^*	
MANUFACTURER	IGT (Australia) Pty Ltd	
CATEGORY	GSS	
SPECIFICATION OR
SERIAL NUMBER	18-SET03	
APPLICATION REFERENCE NUMBER	18-A1175/S01	
TECHNICAL STANDARDS	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
SUBMISSION STANDARDS	NS 10.0 + NSW Appendix (dated 14/01/09)	
^Operational Conditions:  
1.	The system VIP functionality must be disabled during installation.
2.	The system must be fitted with a compliance plate.
3.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine.
4.	The system is approved for use in a local area network (LAN) configuration only.
5.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS).  The UPS must have sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption.  Desirably the system should be equipped wit a “Smart” UPS capable of automatically shutting the system down in the case of a power failure.
*Note: 	The “Ticket In” and “Cashless” facilities are not approved in the ACT.

SYSTEM/DEVICE NAME	Interface Board (iBoard)^* 	
MANUFACTURER	IGT (Australia) Pty Ltd	
CATEGORY	SF 	
SPECIFICATION OR
SERIAL NUMBER	N/A	
APPLICATION REFERENCE NUMBER	18-A1167/S01	
TECHNICAL STANDARDS	NS 9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard V4.18	
SUBMISSION STANDARDS	NS 9.0 + NSW Appendix (dated 23/03/07)	
^Note:	The interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine.
*Note: 	The “Ticket In” and “Cashless” facilities are not approved in the ACT.

SYSTEM/DEVICE NAME	sbNexGen*	
MANUFACTURER	IGT (Australia) Pty Ltd	
CATEGORY	SF (Subsidiary Function)	
SPECIFICATION OR
SERIAL NUMBER	N/A	
APPLICATION REFERENCE NUMBER	18-A1159/S01	
TECHNICAL STANDARDS	NS 9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2,
TITO Technical Standard 4.18	
SUBMISSION STANDARDS	NS 9.0 + NSW Appendix (dated 23/03/07)	
*Note: 	The “Ticket In” and “Cashless” facilities are not approved in the ACT.