Australian Capital Territory
Gaming Machine (Peripheral Equipment) Approval 2010 (No 12)
Notifiable instrument NI2010– 419
made under the  
Gaming Machine Act 2004, section 69 (Approval of gaming machines and peripheral equipment)

1	Name of instrument
This instrument is the Gaming Machine (Peripheral Equipment) Approval 2010 (No 12).

2	Commencement 
This instrument commences the day after the date of notification.

3	Approval
I approve the peripheral equipment described in the attached Schedule to this instrument.  

James Mullan
Delegate
ACT Gambling and Racing Commission

26 July 2010

System/Device Name	Thin Client ATA Graphics Server	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	Gaming Machine (GM)	
GM Type	Graphics Server	
Specification 	1.SES01	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW Jackpot Technical Standards Rev 1.1	
List of Additional Games Suitable for Operation on the Hyperlink LPJS:	
Game Name 	Spec Number	Program ID	
Bone Bonus (Bonus Link)	 1.HF006	 10260861	
Lucky Count (Bonus Link)	 1.HF008	 10160858	
Jungle Joe Searching High and Low (Bonus Link)	 1.HF009	 10260912	
Fire Light - Power Pay (Bonus Link)	 1.HF010	 10160943	
Fortune Princess (Bonus Link)	 1.HF011	 10160753	
Dolphin Magic - Power Pay (Bonus Link)	 1.HF012	 10160944	
Sirena’s Gold (Bonus Link)	 1.HF013	 10160945	
Crusader’s Heart – Power Pay (Bonus Link)	 1.HF014	 10260856	
5 Dragons (Fa Fa Fa)	 1.HF005	 10160917	
Specific Approval Conditions
1.	The Acres Doli Protocol functionality is not a subject of this approval. 
2.	The number of Jackpot Levels displayed by the ATA Graphics Server of a selected Mystery Link should match the number of Jackpot Levels configured in the Jackpot Controller. 	
Operational Conditions
1.	The Thin Client ATA Graphics Server must be connected to an approved Standard / Hyperlink / Random Link Progressive Jackpot. 
2.	The Thin Client ATA Graphics Server active external I/O ports must be housed in a security cage fitted with a security seal to prevent connection or removal of data cables. 	
Application Reference Number	01-A1175/S01	

System/Device Name	IGT Systems Club 	
Manufacturer	IGT (Australia) Pty Ltd	
Category	Subsidiary Equipment 	
Specification 	18-SET02	
System Description	Data Gathering, Report Generating, Player Tracking / Bonus Points and Ticket In  Ticket Out Validation	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard 4.18	
System Software Identifier	Version 3.2	
Maximum Number of Connected Gaming Machines per Transaction Server	
300	
System Details	
System Name	eCash Redemption Terminal	
Specification Number 	18.SER01	
Category	Gaming Support Systems	
Submission Standards	NS9.0 + NSW Appendix (dated 23/03/07)	
Technical Standards	NS9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Operational Conditions
1.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine. 
2.	The system is approved for use in a local area network (LAN) configuration only. 
3.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS). The UPS must have sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption. Desirably the system should be equipped with a “Smart” UPS capable of automatically shutting the system down in the case of a power failure. 	
Application Reference Number	18-A1192/S01