Australian Capital Territory
Gaming Machine (Peripheral Equipment) Approval 2011 (No 6)
Notifiable instrument NI2011– 114
made under the  
Gaming Machine Act 2004, section 69 (Approval of gaming machines and peripheral equipment)

1	Name of instrument
This instrument is the Gaming Machine (Peripheral Equipment) Approval 2011 (No 6).

2	Commencement 
This instrument commences the day after the date of notification.

3	Approval
I approve the peripheral equipment described in the attached Schedule to this instrument.  

Lesley Maloney
Delegate
ACT Gambling and Racing Commission

1 March 2011

Monitoring System Machine Communication Interface “MCI” Software Bugfix	
Device Name	MCI (Machine Communication Interface)	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	SE (Subsidiary Equipment)	
Gaming Machine Type	SEI (Subsidiary Equipment Interface Card)	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS Rev 2.2
TITO Technical Standard Version 4.18	
Software Details	
Device	Software ID	Device Type	Pos	Ver.	CRC32	
MCI 225	MCIXC225.BIN	EPROM	U4	2.25	C694EF55	
The above identified MCI version 2.25 is approved to operate with the following approved monitoring system:	
System Name	SYSTEM 7000	
Category	SE (Subsidiary Equipment)	
Specification Number	01-SET06 & 01-SEZ07	
System Software Identifier	7.2.100.26 and above	
Submission Standards	NS 10.0 + NSW Appendix dated 14/01/09	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard Version 4.18 	
Operational Conditions
1.	The machine communication interface card must be housed in a sealed enclosure, which requires access to the secure area of the Gaming Machine.
2.	The “Ticket In” and “Cashless” facilities are not approved in the ACT.	
Application Reference Number	01-A1228/S01	

Monitoring System “System 7000” Software Bugfix	
System Details 1	SYSTEM 7000	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	SF (Supporting Function)	
Specification Number	01-SET06 & 01-SEZ07	
System Software Identifier	7.3.0.1	
Submission Standards	NS 10.0 + NSW Appendix dated 14/01/09	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard V4.18 	
Software Details 1	
File Name	System 7000 Floor Server Description	Version	CRC 32	
Dacom Install	Dacom-install-5.31.tar	5.31	c098e5e8	
Install Dacom	Install-dacom-5.31.zip	5.31	f062f4fc	
Master	Master-5.31.zip	5.31	6b9f00cd	
System Details 2	
System Name 	SYSTEM 7000	
Category	SF (Supporting Function)	
Specification Number	01-SET06 & 01-SEZ07	
System Software Identifier	7.2.100.26	
Submission Standards	NS 10.0 + NSW Appendix dated 14/01/09	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard V4.18 	
Software Details 2				
File Name	System 7000 Floor Server Description	Version	CRC 32	
Dacom Install	Dacom-install-5.23.tar	5.23	D1169DFD	
Install Dacom	Install-dacom.zip	5.23	B737188D	
Master	Master-5.23.zip	5.23	4F7A9489	
Operational Conditions
1.	The “Ticket In” and “Cashless” facilities are not approved in the ACT.	
Application Reference Number	01-A1227/S01	

Standard Linked Progressive Jackpot System Jackpot Parameter Update	
System Name	Standard LPJS	
Manufacturer	IGT (Australia) Pty Ltd	
Category	PC (Progressive Controller)	
PC Type	STD (Standard Progressive Controller)	
Specification Number	18.YA008	
LPJS Description	4 level Standard Linked Progressive Jackpot Controller and Interface Card with CCCE Port Sharing Functionality	
Technical Standards
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standards Rev 1.1	
Controller Firmware	Version 3.08	
Interface Card Firmware	Version 1.21	
Jackpot Themes	Wheel of Gold	
Operational Conditions
1.	The Paltronics Controller and Subsidiary Equipment Interface Card with specified firmware must operate as part of the IGT Standard Linked Progressive Jackpot System with the “Wheel of Gold” jackpot theme.
2.	The above-mentioned Jackpot Controller / SEI firmware must operate in conjunction with the “Wheel of Gold” game / shell combination.
3.	When using an overhead display with the VGA Display Driver, the following conditions must be complied:
a)	The system is to be run only under Windows XP operating system.
b)	The keyboard and mouse is to be attached only when performing maintenance and must be removed at all other times.
c)	The PC housing must have a provision to seal all points where the controller cables may be disconnected.
d)	The write filter application must be loaded on the hard drive at start up.
4.	The system interface card must be enclosed in a sealed enclosure.	
Application Reference Number	18-A1215/S01