Australian Capital Territory
Gaming Machine (Peripheral Equipment) Approval 2011 (No 15)
Notifiable instrument NI2011–454
made under the  
Gaming Machine Act 2004, section 69 (Approval of gaming machines and peripheral equipment)

1	Name of instrument
This instrument is the Gaming Machine (Peripheral Equipment) Approval 2011 (No 15).

2	Commencement 
This instrument commences the day after the date of notification.

3	Approval
I approve the peripheral equipment described in the attached Schedule to this instrument.  

Lesley Maloney
Delegate
ACT Gambling and Racing Commission

10 August 2011

Updated Standard Linked Progressive Jackpot System and Optional VGA Display Driver	
Device Name	Standard LPJS	
Manufacturer	Ainsworth Game Technology Limited	
Specification Number	44.YA005	
Category	PC (Progressive Controller)	
Category Type	STD (Standard Progressive Controller)	
Technical Standards 
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standard Rev 1.2	
Controller Firmware	Version 02.00.03.08	
Interface Card Firmware	Version 1.44	
Jackpot Theme	Rio Grande Rapids (Single Level)	
Operational Conditions
1.	The Paltronics Controller and Subsidiary Equipment Interface Card with specified firmware must operate as part of AGT’s Single Level Standard Linked Progressive Jackpot System with the ‘Rio Grande Rapids’ game theme.
2.	The above-mentioned Jackpot Controller / SEI firmware must operate in conjunction with an AGT’s Single Level ‘Rio Grande Rapids’ game / shell combination.
3.	The system interface card must be enclosed in a sealed enclosure.
4.	When using an overhead display with the VGA Display Driver, the following conditions must be complied:
a)	The system is to be run only under Windows XP operating system.
b)	The keyboard and mouse is to be attached only when performing maintenance and must be removed at all other times.
c)	The PC housing must have a provision to seal all points where the controller cables may be disconnected.
d)	The write filter application must be loaded on the hard drive at start up.	
Application Reference No.	44-A0648/S01; 44-A0643/S01