Australian Capital Territory
Gaming Machine (Peripheral Equipment) Approval 2013 (No 4)
Notifiable instrument NI2013– 248
made under the  
Gaming Machine Act 2004, section 69 (Approval of gaming machines and peripheral equipment)

1	Name of instrument
This instrument is the Gaming Machine (Peripheral Equipment) Approval 2013 (No 4).

2	Commencement 
This instrument commences the day after the date of notification.

3	Approval
I approve the peripheral equipment described in the attached Schedule to this instrument.  

Lesley Maloney
Delegate
ACT Gambling and Racing Commission

28 May 2013

Updates for  Link Progressive Jackpot System 	
Manufacturer	Ainsworth Game Technology Ltd	
Category	Progressive Controller	
System Name 	A560 Link Progressive Jackpot System	
Specification Number	44.YC000 – Random (Mystery) LPJS
44.YA007 – Standard LPJS	
Submission Standards
Technical Standards	NS 10.1 + NSW Appendix (dated 24/11/11)
NSW CPTS 2.3; NSW Jackpot TS Rev 1.2
TITO Technical Standard V4.20	
LPJS Description	Random and Standard Linked Progressive Jackpot Controller with CCCE Jackpot Transfer Port Sharing functionality	
Controller Software version	X211761ED	
Additional Random Progressive Jackpot Themes	a)	Big Time
b)	Firestrike	
Software details	
Description	Firmware ID	
LPJS Controller	
Link Controller Game	NXC0201A	
Display Media (optional)	NXD0201C	
Display Controller	
Display Media (optional)	NXD0201C	
Specific Approval Conditions
1.	The A560 link Progressive Jackpot System is approved to configure up to 8 progressive jackpot groups only.
2.	The supplier must ensure that for each progressive Jackpot Group enrolled on the A560 Link Progressive Jackpot System, a new serial number is assigned.
3.	If Double Shot Favourites Standard Progressive is configured, the Display Controller with Media firmware version ‘NXD0181B’ must be enabled.	
Application Reference Numbers	44-A0788/S03	

Monitoring System Software Update and New Subsidiary Equipment Interface Card	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	Subsidiary Equipment	
System Name 1	System 7000	
System Description
Data Gathering, Report Generating, Player Tracking / Bonus Points and Ticket In Ticket Out Validation, Dual Port Reconciliation, Take a Break, Extended Floor Configuration, Pre-commitment and Popup Messages.	
Specification Number	1.SET06	
System Name 2	System 7000	
System Description
Data Gathering, Report Generating, Player Loyalty / Bonus Points Pre-commitment and Popup Messages. 	
Specification Number	1.SEZ07	
Submission Standards
Technical Standards	NS 10.1 + NSW Appendix (dated 24/11/11)
NSW CPTS 2.3; TITO Technical Standard V4.20	
System software Identifier	7.3.0.10 Single-site
7.3.0.10 Multi-site (Extended Floor Conf)	
Interface card software details	
Device	Software ID	
Player Marketing Module (PMM Mk7)	
PMM Mk7	PMM7-4.03.bin	
PMM Mk7	PMM7-4.03.pof	
System Name 3	System 7000 – Remote Site	
System Description
Data Gathering, Report Generating, Player Tracking / Bonus Points, Ticket In Ticket Out Validation, Dual Port Reconciliation, Take a Break, Extended Floor Configuration, Pre-commitment and Popup Messages.	
Specification Number	1.SET07	
System software Identifier	7.3.0.10 Multi-site 	
Submission Standards
Technical Standards	NS 10.1 + NSW Appendix (dated 24/11/11)
NSW CPTS 2.3; TITO Technical Standard V4.20	
Interface card software details	
Device	Software ID	
Player Marketing Module (PMM Mk7)	
PMM Mk7	PMM7-4.03.bin	
PMM Mk7	PMM7-4.03.pof	
The above-identified System 7000 is approved to operate with the following approved cash redemption terminals	
Device Name 1	Sprintquip Cashback Centre	
Specification Number	1.SER00	
Software Version	TRMD4_09_0K5.S19	

Device Name 2	Sprintquip Ultra Centre	
Category	Subsidiary Equipment	
Specification Number	1.SER01	
Software Version	1.0.0.358	
Device Name 3	ecash Cash Redemption Terminal	
Specification Number	69.SER00	
Software Version	V2.3.41.80	
Application Reference Number	01-A1408/S01 	

Alternate ATA Graphics Server 	
Device Name	Kontron ATA Graphics Server	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	Gaming Machine	
Category Type	Graphics Server	
Specification Number	1.SES03	
Submission Standards
Technical Standards	NS 10.1 + NSW Appendix (dated 24/11/11)
NSW CPTS 2.3; NSW Jackpot TS Rev 1.2	
LPJS Details 1 – Random          with Mk6 and Gen7 platforms	
LPJS Type	Software Version	Specification Number	
Mikohn LPJS	CCCE44	32.YC000	
Paltronics LPJS	52XO199C / 52XE199C	52.YC000	
	XST0207O / XST0207E	52.YC000	
Paltronics LPJS	XSE0116O / XSE0116E	52.YC001	
LPJS Details 2 – Hyperlink        with Mk6 and Gen7 platforms	
LPJS Type	Software Version	Specification Number	
Hyperlink LPJS	SHL0328O / SHL0328E	1.YA000
1.YH030
1.YH050
1.YH060 to 1.YH170	
	a)	SHL0330O / SHL0330E
b)	SHL0332O / SHL0332E	1.YA000
1.TH030
1.YH050
1.YH060 to 1.YH170
1.YH280
1.YH290 TO 1.YH310	
	SHL0335O / SHL0335E	1.YH000
1.YH030
1.YH050
1.YH060 to 1.YH170
1.YH280
1.YH290 to 1.YH310
1.YH320
1.YHD00	
	SHL0404O / SHL0404E	1.YA001	
	SHL0501O / SHL0501E	1.YA002	
	SHL0502O / SHL0502E	1.YA002	
	SHL0505O / SHL0505E	1.YA002	
	SHL0600O / SHL0600E	1.YA002	
	SHL0603O / SHL0603E	1.YA002	
	SHL0604O / SHL0604E	1.YA002	

LPJS Details 3 – Standard         with Gen7 platforms	
LPJS Type	Software Version	Specification Number	
Standard LPJS	SHL0404O / SHL0404E	1.YA001	
	SHL0603O / SHL0603E	1.YA002	
	SHL0604O / SHL0604E	1.YA002	
Platform / Cabinet Details	
a)	Overhead Display Connection Only	
Mk 6 	Mk 6 Xcite – Low Boy, Casino Top (Configured with either Hopper and or Ticket Printer option)
Slant Mk 6 – Round Top (Configured with Ticket Printer only)	
Gen7	Gen7 Viridian – Chop Top (Configured with either Hopper and or Ticket Printer option)
Gen7 Upgrade XCite – Lowboy (Configured with either Hopper and or Ticket Printer option)
Gen7 Viridian Widescreen – Chop Top (Configured with either Hopper and or Ticket Printer option)	
b)	Overhead Display + Top Box LCD Monitor Connection	
Mk 6	Mk 6 XCite – Low Boy (with external LCD) (Configured with either Hopper and or Ticket Printer option)
Mk 6 (XTreme) – Casino Top (with in-machine LCD) (Configured with either Hopper and or Ticket Printer option)
Slant Mk 6 – Casino Top (with in-machine LCD) (Configured with Ticket Printer only)	
Gen7	Gen7 Viridian – Casino Top (with –in-machine LCD)(Configured with either Hopper and or Ticket Printer option)
Gen7 Slant – Casino Top (with –in-machine LCD) (Configured with Ticket Printer only)
Gen7 Upgrade XCite – Lowboy (with external LCD) (Configured with either Hopper and or Ticket Printer option) 
Gen7 Upgrade XTreme – Casino Top (with –in-machine LCD)(Configured with either Hopper and or Ticket Printer option)
Gen7 Viridian Widescreen – Casino (with –in-machine LCD) (Configured with Ticket Printer only)
Gen7 Vii Slant – Casino Top (with –in-machine LCD) (Configured with Ticket Printer only)	
Previously approved games suitable for operation with this ATA Graphics Server	All games previously approved for operation with the above-mentioned jackpot controllers are suitable for operation with the Kontron ATA Graphics Server.	

Specific Approval Conditions
1.	Each Kontron ATA Graphics Server operating within a venue must be authorised with the corresponding Specification Number.
2.	The Kontron ATA Graphics Server must be connected to an approved Standard / Hyperlink / Random Linked Progressive Jackpot System as given above.
3.	The Kontron ATA Graphics Server active external I/O ports must be housed in a cage fitted with a security seal to prevent connection or removal of data cables.
4.	The Acres Doli Protocol functionality is not a subject of this approval.
5.	The display content and access to display parameters must be implemented in a secure manner to prevent unauthorised access.  That is, access is limited to authorised Aristocrat personnel or authorised Aristocrat agents.
6.	The display is not to be used for the purpose of advertising or promotions.
7.	The jackpot pool values are to be displayed to the players generally most of the time (i.e. the display must keep players informed of the current state of the jackpot(s)).
8.	The number of jackpot levels displayed by the Kontron ATA Graphics Server of a selected Mystery Link should match the number of jackpot Levels configured in the Jackpot Controller.
9.	The display is not to be used for feature or bonus games.
10.	The display material is not to be offensive and harm minimisation must be considered.	
Application Reference Numbers	01-A1390/S01