Australian Capital Territory
Gaming Machine (Peripheral Equipment) Approval 2013 (No 7)
Notifiable instrument NI2013–448
made under the  
Gaming Machine Act 2004, section 69 (Approval of gaming machines and peripheral equipment)

1	Name of instrument
This instrument is the Gaming Machine (Peripheral Equipment) Approval 2013 (No 7).

2	Commencement 
This instrument commences the day after the date of notification.

3	Approval
I approve the peripheral equipment described in the attached Schedule to this instrument.  

Lesley Maloney
Delegate
ACT Gambling and Racing Commission

26 September 2013

Alternate Hardware Assembly for the A560 LPJS Controller	
Device Name	A560 Link Progressive Jackpot System	
Manufacturer	Ainsworth Game Technology Limited	
Specification Number	44.YC000 – Random (Mystery) LPJS
44.YA007 – Standard LPJS	
Category	Progressive Controller	
Technical Standards	NS 10.1 + NSW Appendix (dated 24/11/11)
NSW CPTS 2.3; TITO Technical Standard V4.20
NSW Jackpot Technical Standard Rev 1.2	
Submission Standards	NS 10.3 + NSW Appendix (dated 24/04/13)	
Hardware Details	
Device Name	Device Part Number	
Alternate A560 LC Power Supply	220425	
Application Reference No.	44-A0800/S01	

Subsidiary Equipment Interface Card	
System/Device Name	iBoard	
Manufacturer	IGT (Australia) Pty Ltd	
Category	Subsidiary Equipment Interface Card	
Technical Standards	NSW CPTS 2.3; TITO Technical Standard V4.20	
Submission Standards	NS10. + NSW Appendix (dated 24/11/11)	
Software Details	
Device Name	File Name	Version	Media	CRC-32	
Interface Card – iBoard	iBoard.jar	140344	FLASH	D0899A80	
This subsidiary equipment interface card is approved to operate with the following systems.	
System details 1		
System Name	IGT Systems Club	
Specification number	18.SET02	
System Software version	3.6 SP9 and later	
System details 2		
System Name	IGT Systems Club – Remote Site	
Specification number	18.SET04	
System Software version	3.6 SP9 and later	
Application Reference Number	18-A1258/S01	

Updated Standard Linked Progressive Jackpot System 	
System Name	Standard LPJS	
Manufacturer	IGT (Australia) Pty Ltd	
Category	Progressive Controller	
Type	Standard Progressive Controller	
Specification Number	18.YA009	
Submission Standards
Technical Standards	NS 10.1 + NSW Appendix (dated 24/11/11)
NSW CPTS 2.3; NSW Jackpot TS Rev 1.2	
LPJS Description	1 Level Standard Linked Progressive Jackpot Controller and Interface Card with CCCE Port Sharing Functionality.	
Controller Firmware	Version 3.08	
Interface Card Firmware	Version 1.21	
Jackpot Themes	Jetsetter Link	
Specific Approval Conditions
1.	The Paltronics Controller and Subsidiary Equipment Interface Card with specified firmware must operate as part of the IGT Standard Linked Progressive Jackpot System with the “Jetsetter Link” jackpot theme.
2.	The above-mentioned Jackpot Controller / SEI firmware must operate in conjunction with a “Jetsetter Link” game / shell combination.
3.	When using an overhead display with the VGA Display Driver, the following conditions must be applied:
a)	The system is to be run only under Windows XP operating system.
b)	The keyboard and mouse is to be attached only when performing maintenance and must be removed at all other times.
c)	The PC housing must have a provision to seal all points where the controller cables may be disconnected.
d)	The write filter application must be loaded on the hard drive at start up.
4.   The system interface card must be enclosed in a sealed enclosure.	
Application Reference Numbers	18-A1251/S03	

Updated Standard Linked Progressive Jackpot System 	
System Name	Standard LPJS	
Manufacturer	IGT (Australia) Pty Ltd	
Category	Progressive Controller	
Type	Standard Progressive Controller	
Specification Number	18.YA009	
Submission Standards
Technical Standards	NS 10.1 + NSW Appendix (dated 24/11/11)
NSW CPTS 2.3; NSW Jackpot TS Rev 1.2	
LPJS Description	1 Level Standard Linked Progressive Jackpot Controller and Interface Card with CCCE Port Sharing Functionality.	
Controller Firmware	Version 3.08	
Interface Card Firmware	Version 1.21	
Jackpot Themes	Jetsetter Link 2	
Specific Approval Conditions
1.	The Paltronics Controller and Subsidiary Equipment Interface Card with specified firmware must operate as part of the IGT Standard Linked Progressive Jackpot System with the “Jetsetter Link 2” jackpot theme.
2.	The above-mentioned Jackpot Controller / SEI firmware must operate in conjunction with a “Jetsetter Link 2” game / shell combination.
3.	When using an overhead display with the VGA Display Driver, the following conditions must be applied:
a)	The system is to be run only under Windows XP operating system.
b)	The keyboard and mouse is to be attached only when performing maintenance and must be removed at all other times.
c)	The PC housing must have a provision to seal all points where the controller cables may be disconnected.
d)	The write filter application must be loaded on the hard drive at start up.
4.   The system interface card must be enclosed in a sealed enclosure.	
Application Reference Numbers	18-A1252/S03