Australian Capital Territory
Gaming Machine (Peripheral Equipment) Approval 2014 (No 8)
Notifiable instrument NI2014– 434
made under the  
Gaming Machine Act 2004, section 69 (Approval of gaming machines and peripheral equipment)

1	Name of instrument
This instrument is the Gaming Machine (Peripheral Equipment) Approval 2014 (No 8).

2	Commencement 
This instrument commences on the day after its notification.

3	Approval
I approve the peripheral equipment described in the attached Schedule to this instrument.  

4	Revocation
This instrument revokes:

•	NI2010-19	•	NI2010-231	•	NI2010-569	
•	NI2010-46	•	NI2010-248	•	NI2010-580	
•	NI2010-112	•	NI2010-274	•	NI2010-611	
•	NI2010-159	•	NI2010-310	•	NI2010-643	
•	NI2010-184	•	NI2010-355	•	NI2010-649	
•	NI2010-211	•	NI2010-419	•	NI2010-656	

James Mullan
Delegate
ACT Gambling and Racing Commission

28 August 2014

SYSTEM/DEVICE NAME	Multi Venue Jackpot System^	
MANUFACTURER	Paltronics Australia Pty Ltd	
CATEGORY	Subsidiary Equipment	
SYSTEM DESCRIPTION	999 Jackpot Levels Multi Venue Linked Progressive Jackpot System with CCCE Jackpot Transfer and Dual Port functionality with up to 500 (100 unless communications systems have been tested) Inter-Venue Jackpot Linked Gaming Machines	
APPLICATION REFERENCE NUMBER	ACT:SC/26-A0001	
TECHNICAL STANDARDS	NS 9.0 + NSW Appendix (dated 23/3/07)
NSW Jackpot TSR1.1; NSW CPTS 2.2
	
SUBMISSION STANDARDS	NS 9.0 + NSW Appendix (dated 23/03/07)	

SYSTEM/DEVICE NAME	Multi Venue Jackpot System – Local Jackpot Controller^	
MANUFACTURER	Paltronics Australasia Pty Ltd	
CATEGORY	Subsidiary Equipment	
SYSTEM DESCRIPTION	64 Jackpot Levels Mystery Linked Progressive Jackpot System with CCCE Jackpot Transfer and Dual Port functionality with 200 Attached Gaming Machines	
APPLICATION REFERENCE NUMBER	ACT:SC/26-A0001	
TECHNICAL STANDARDS	NS 9.0 + NSW Appendix (dated 23/3/07)
NSW Jackpot TSR1.1; NSW CPTS 2.2	
SUBMISSION STANDARDS	NS 9.0 + NSW Appendix (dated 23/03/07)	
Operational Conditions
1)	The logic cage(s) housing the logic boards and other sensitive components of the MVJS (the MVJS Server and each attached local jackpot controller) must be closed and key-locked at all times, except during system maintenance or upgrade of the MVJS.
2)	The MVJS logic cages’ lock key(s) must be under the control of the venue manager.
3)	The MVJS must be configured to use a different session encryption key every 24 hours or more frequently. The session encryption key is the “password” used by the MVJS to encrypt all its communications between the MVJS Server, Local Jackpot Controllers and Config/Console Workstations.
4)	The ability to perform any server administration, system configuration, software modification and/or control the servers’ operation remotely must be disabled at all times, except during system maintenance or upgrade of the MVJS.
5)	Dedicated communication line (physical or logical) must be used for all communications between the MVJS Server, Local Jackpot Controllers and Config/Console Workstations.
6)	‘Rolled-up turnover’ is not approved for use in ACT and must be disabled at all times.
7)	‘Offline play’ is not approved for use in ACT and must be disabled at all times. The parameters “Maximum Offline Play Time” and “Maximum Offline Turnover” must be set to zero for each operating jackpot level.
8)	The supplier must limit the number of inter-venue gaming machines operating with an MVJS to 100 unless the testing outlined in the OLGR Application Testing Report is carried out prior to increasing the number of inter-venue gaming machines. Please note that licensees cannot increase the number of gaming machines operated with an MVJS unless they have sought an amendment to their Multi User Permit.	

SYSTEM/DEVICE NAME	IGT Systems Club Release 3.1b (ARN18-A1183/S01)	
MANUFACTURER	IGT (Australia) Pty Ltd	
CATEGORY	Subsidiary Equipment	
SPECIFICATION OR
SERIAL NUMBER	18-SET02	
SUBMISSION STANDARDS	NS10.0 + NSW Appendix (dated 14/01/09)	
TECHNICAL STANDARDS	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard 4.18	
Maximum number of connected gaming machines per Transaction Server is 300.	
The IGT Systems Club Release 3.1b is approved to operate with the following approved eCash Redemption Terminal specification number 18-SER01	
OPERATIONAL CONDITIONS
1.	The system VIP functionality must be disabled during installation.
2.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine.
3.	The system is approved for use in a local area network (LAN) configuration only.
4.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS).  The UPS must have sufficient capacity to allow the system and any associated critical elements, to be shut down gracefully in the event of a power interruption.  Desirably the system should be equipped with a “Smart” UPS capable of automatically shutting the system down in the case of a power failure. 	
APPLICATION REFERENCE NUMBER	18-A1183/S01	

System Device Name	ATA Graphics Server
Thin Client ATA Graphics Server	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	Gaming Machine	
Gaming Machine Type	Other (Graphics Server)	
Specification Number	1.SES00
1.SES01	
Technical Standards	NSW Jackpot Technical Standards Rev 1.1	
Specific Approval Conditions
1.	The Acres Doli Protocol functionality is not a subject of this approval.
2.	The number of Jackpot Levels displayed by the ATA Graphics Server of a selected Mystery Link should match the number of Jackpot Levels configured in the Jackpot Controller.	
Operational Conditions
1.	Each ATA Graphics Server (P/N: 57783) operating within a venue must be authorised with the Specification Number: 1.SES00.
2.	Each Thin Client ATA Graphics Server (P/N: 442004 or 442027_2) operating within a venue must be authorised with the Specification Number: 1.SES01.
3.	The ATA Graphics Server or Thin Client ATA Graphics Server must be connected to an approved Standard / Hyperlink / Random Link Progressive Jackpot System as given above.
4.	The ATA Graphics Server or Thin Client ATA Graphics Server active external I/O ports must be housed in a security cage fitted with a security seal to prevent connection or removal of data cables.	
Application Reference Number	01-A1134/S01	

System Device Name	Sprintquip Cashback Centre	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	Subsidiary Equipment	
Specification Number	01-SER00	
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2; TITO Technical Standard V4.18	
Application Reference Number	01-A1142/S01	

Manufacturer	Aristocrat Technologies Australia Pty Ltd	
System Details 1	
System Name	System 7000	
System Description	Data Gathering, Report Generating, Player Tracking / Bonus Points and Ticket In Ticket Out Validation, Dual Port Reconciliation and Take A Break	
Category Type	Subsidiary Equipment	
Specification 	01-SET06	
System Details 2	
System Name	System 7000	
System Description	Data Gathering, Report Generating and Player Tracking / Bonus Points	
Category Type	Subsidiary Equipment	
Specification	01-SEZ07	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard 4.18	
The above identified System 7000 is approved to operate with the following approved cash redemption terminal	
System Name	Sprintquip Cashback Centre	
System Description	Gaming Machines Printed Ticket Redemption Station	
Category	Subsidiary Equipment	
Specification 	01-SER00	
Submission Standards	NS9.0 + NSW Appendix (dated 23/03/07)	
Technical Standards	NS9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard 4.18	
Operational Conditions
The subsidiary equipment interface card must be housed in a sealed enclosure, which requires access to the secure area of the Gaming Machine	
Application Reference Number	01-A1148/S01	

System Name	IGT Systems Club	
Manufacturer	IGT (Australia) Pty Ltd	
System Description	Data Gathering, Report Generating, Player Tracking / Bonus Points and Ticket In Ticket Out Validation	
Category Type	Subsidiary Equipment	
Specification 	18-SET02	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard 4.18	
The IGT Systems Club Version 3.1i is approved to operate with the following approved eCash Redemption Terminal:	
System Name	eCash Redemption Terminal	
System Description	Gaming Machines Printed Ticket Redemption Station	
Category	Gaming Support Systems	
Specification 	18-SER01	
Submission Standards	NS9.0 + NSW Appendix (dated 23/03/07)	
Technical Standards	NS9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard 4.18	
Operational Conditions
1.	The system VIP functionality must be disabled during installation
2.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine
3.	The system is approved for use in a local area network (LAN) configuration only
4.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS). The UPS must have sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption. Desirably the system should be equipped with a “Smart” UPS capable of automatically shutting the system down in the case of a power failure	
Application Reference Number	01-A1186/S01, S02	

System Name	Standard LPJS – Mystical Temple 	
Manufacturer	Konami Australia Pty Ltd	
System Description	3 Levels Standard Linked Progressive Jackpot System with CCCE Transfer	
Category Type	Subsidiary Equipment	
Specification 	39-YA002	
Submission Standards	NS9.0 + NSW Appendix (dated 23/03/07)	
Technical Standards	NS9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
NSW Jackpot TS Rev 1.1	
Operational Conditions
The system interface card must be enclosed within a sealed enclosure	
Application Reference Number	39-A0800/S01, /S02, /S03	

System/Device Name	Hyperlink LPJS	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	PC	
Category Type	STD (Standard Progressive Controller)	
Specification 	1.YA002	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard 4.18
NSW Jackpot Technical Standards Rev 1.1	
Operational Conditions
1.	The ATA Graphics Server (1.SES00) or Thin Client ATA Graphics Server (1.SES01) must be connected to the above mentioned Hyperlink Link Progressive Jackpot  System)
2.	There should be at least one venue overhead display connected to the ATA Graphics Server (1.SES00) or Thin Client ATA Graphics Server (1.SES01) so as to display pool values, the GMID / House Number of the winning gaming machine, jackpot win amounts and the G-Line message. 	
Application Reference Number	A1153/S01	

System/Device Name	Hyperlink LPJS	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	PC	
Category Type	STD (Standard Progressive Controller)	
Specification 	1.YA002	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18
NSW Jackpot Technical Standards Rev 1.1	
Jackpot Themes	Jaws Link
Bonus Link
Fa Fa Fa Link	
Operational Conditions
1.	The ATA Graphics Server (1.SES00) or Thin Client ATA Graphics Server (1.SES01) must be connected to the above mentioned Hyperlink Link Progressive Jackpot System.
2.	There should be at least one venue overhead display connected to the ATA Graphics Server (1.SES00) or Thin Client ATA Graphics Server (1.SES01) so as to display pool values, the GMID / House Number of the winning gaming machine, jackpot win amounts and the G-Line message. 	
Application Reference Number	A1159/S01	

System/Device Name	Coin Validator	
Manufacturer	Shuffle Master Australasia Pty Ltd 	
Category	Gaming Machine	
Category Type	Hardware Component	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2	
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2	
Platform/Cabinet
PC3 –  High Top, Casino Top, Casino Plus Top, Low Top
eStar – Round Top, Square Top, Low Top
             Round Top with Mystery Link LCD 
             Square Top with Mystery Link LCD
             Round Top (with in-machine 17” LCD)
eStar PC4 – Round Top, Square Top, Low Top
                     Round Top (with in-machine 17” LCD)	
Application Reference Number	35-A0639/S01	

System/Device Name	IGT Systems Club (bugfix)	
Manufacturer	IGT (Australia) Pty Ltd	
Category	Subsidiary Equipment	
Specification Number	18-SET02	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard 4.18	
The IGT Systems Club Version 3.1J is approved to operate with the eCash redemption Terminal, specification number 18.SER01.	
Operational Conditions  
1.	The system VIP functionality must be disabled during installation.
2.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine.
3.	The system is approved for use in a local area network (LAN) configuration only.
4.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS).  The UPS must have sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption.  Desirably the system should be equipped with a “Smart” UPS capable of automatically shutting the system down in the case of a power failure.	
Application Reference Number	18-A1189/S01	

System/Device Name	Maxetag	
Manufacturer	Global Gaming	
Category	Subsidiary Equipment	
Specification Number 	25-SEP00	
Submission Standards	NS9.0 + NSW Appendix (dated 23/03/2007)	
Technical Standards	NS9.0 + NSW Appendix (dated 23/03/2007) NSW CPTS 2.2	
Application Reference Number	25-A0190/S01, S02	

System/Device Name	Prime Impact	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	Subsidiary Equipment	
Category Type	Subsidiary Equipment Interface	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard 4.18	
The following systems are approved to operate with the above-identified subsidiary equipment interface card “Prime Impact Version 1.18”.	
System Details 1:	
System Name	System 6000	
Specification Number	01-SEBT0, 01-SET05 & 01-SEBZ06	
System Details 2:	
System Name	System 7000	
Specification Number	01-SET06 & 01-SEZ07	
Operational Conditions
The subsidiary equipment interface card must be housed in sealed enclosure, which requires access to the secure area of the Gaming Machine.	
Application Reference Number	01-A1170/S01	

System/Device Name	Central Credit Unit Model 5.5T	
Manufacturer	Global Gaming Pty Ltd	
Specification Number	25-SET02	
Category	Subsidiary Equipment	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard 4.18	
The Central Credit Unit Model 5.5T is not approved to operate with the eCash Redemption Terminal (specification number 25.SER00) in the ACT.	
Specific Approval Conditions
Global Gaming Industries (GGI) must inform each purchaser and/or lessee of the Central Credit Unit Model 5.5T (CCU Model 5.5T) in writing prior to or at the time of purchase/lease that the CCU Model 5.5T is a ‘line of sight’ centralised cash control system and if all the gaming machines are not visible from the cashier station (by some means), there is an increased risk of player complaints/disputes in respect of transferring money to/out of the gaming machines from/out of the cashiers direct field of view. 	
Operational Conditions
1.	The CCU Model 5.5T must operate with a printer at all times.
2.	When operating in a dual port environment the CCU Model 5.5T must be connected directly to Port P1 of gaming machine using GAME port of the CCU Model 5.5T interface card.
3.	The CCU Model 5.5T interface card must be housed in a sealed enclosure, which requires access to the secure area of the Gaming Machine.
4.	When the CCU Model 5.5T is operated with a Note Dispensing Safe, the note dispensing safe must be located in an area not accessible to the public and shall be operated by venue staff only.
5.	The CCU Model 5.5T is approved to operate in a dual port environment with any approved Integrated Gaming, Mikohn or Paltronics-branded Linked Progressive Jackpot System that support jackpot CCCE transfer capability. 	
Application Reference Number	01-A0192/S01	

System/Device Name	Bill Acceptor – MEI SC66	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Category	Gaming Machine	
Category Type	Hardware Component	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Platform/Cabinet	GENEX – Midway, Lowboy, G-Deluxe	
Application Reference Number	06-A0277/S01	

System/Device Name	Coin Separator	
Manufacturer	Konami Australia Pty Ltd	
Category	Gaming Machine	
Category Type	Hardware Component	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
System Details 1:	
 Description	Manufacturer’s Model 	Konami’s Part Number	
Coin Validator
 	Microcoin QL, Q7120 
CFG: AU002-A3	 3102002A	
	Microcoin QL, Q7120-DO (RoHS) CFG: AU002_C3; Firmware: V3.98	 3102002A	
2-Way Separator	Microcoin QL, 7003032	 3102003A	
	Microcoin QL, 7003033	 3102003A	
Platform/Cabinet:
Endeavour Series – High Top, Casino Top, Lowboy, Casino Top with LCD, Hex Casino Top with LCD, Casino Top with LPJS, Hex Casino Top with LPJS
Endeavour ES 500 – Casino Top, Lowboy, Casino Top with LCD, Hex Casino Top with LCD, Casino Top with LPJS, Hex Casino Top with LPJS	
System Details 2:	
 Description	Manufacturer’s Model 	Konami’s Part Number	
Coin Validator
	Microcoin QL, Q7120-D
CFG: AU002-C3	 3102002A	
	Microcoin QL, Q7120-DO (RoHS) CFG: AU002_C3; Firmware: V3.98	 3102002A	
2-Way Separator	Microcoin QL, 7003032	 3102003A	
	Microcoin QL, 7003033	 3102003A	
Platform/Cabinet:
K2V – High Top, Casino Top, Lowboy, Casino Top with LCD, Hex Casino Top with LCD
K2V 500 –Casino Top, Lowboy, Casino Top with LCD, Hex Casino Top with LCD
K2V Upgrade – High Top, Casino Top, Lowboy, Casino Top with LCD, Hex Casino Top with LCD
K2V 500 Upgrade – Casino Top, Lowboy, Casino Top with LCD, Hex Casino Top with LCD
K2V Advantage 5 – Casino Top, Casino Top with LCD/LED	
System Details 3:	
 Description	Manufacturer’s Model 	Konami’s Part Number	
Coin Validator	Microcoin QL, Q7120-DO (RoHS) CFG: AU002_C3; Firmware: V3.98	3102002A	
2-Way Separator	Microcoin QL, 7003032	3102003A	
	Microcoin QL, 7003033	3102003A	
Platform/Cabinet:
KGP 2.0 UVS Podium – Upper LCD Box, Tombstone LCD Box, Short Top Box	
Application Reference Number	39-A0867/S01	

System/Device Name	AVP BC20 Platform Update #2	
Manufacturer	IGT (Australia) Pty Ltd	
Category	Gaming Machine	
Category Type	Hardware Component	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Platform / Cabinet Details	AVP BC20 – Video Top	
Application Reference Number	18-A1191/S01	

System/Device Name	IGT Systems Max (Bugfix)	
Manufacturer	IGT (Australia) Pty Ltd	
Category	Gaming Support System	
Specification 	18.SET03	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard 4.18	
System Software Identifier	Release 3.1.0 Service Pack 5 (SP5)	
Operational Conditions
1.	The System must be fitted with a compliance plate. 
2.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine. 
3.	The system is approved for use in a local area network (LAN) configuration only. 
4.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS).  The UPS must have sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption.  Desirably the system should be equipped with a “Smart” UPS capable of automatically shutting the system down in the case of a power failure.
5.	The IGT Systems Max must be configured in such a way that only authorised personnel have access to critical functions and sensitive information contained in the system. 	
Additional Information
The system is approved to operate in a dual port environment with any approved Paltronics Branded Linked Progressive Jackpot Systems that support jackpot CCCE transfer capability. 	
Application Reference Number	18-A1175/S01	

System/Device Name	Sandwich Box Assembly	
Manufacturer	IGT (Australia) Pty Ltd	
Category	Gaming Machine	
Category Type	Hardware Component	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Platform / Cabinet Details
	Game King – High Top, Casino Top, Lowboy
GU4C – Casino Top, Lowboy	
Application Reference Number	18-A1193/S01	

System/Device Name	Marquee Assembly	
Manufacturer	Shuffle Master Australasia Pty Ltd	
Category	Gaming Machine	
GM Type	Hardware Component	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Marquee Assembly	SM P/N: 10-162A
SM P/N: HNS-4809	
Platform / Cabinet Details	eStar – Round Top, Square Top, Low Top
Round Top with Mystery Link LCD
Square Top with Mystery Link LCD
Round Top (with in-machine 17” LCD)
eStar PC4 – Round Top, Square Top, Low Top
        Round Top (with in-machine 17” LCD)	
Application Reference Number	35-A0654/S01	

System/Device Name	Thin Client ATA Graphics Server	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	Gaming Machine (GM)	
GM Type	Graphics Server	
Specification 	1.SES01	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW Jackpot Technical Standards Rev 1.1	
List of Additional Games Suitable for Operation on the Hyperlink LPJS:	
Game Name 	Spec Number	Program ID	
Bone Bonus (Bonus Link)	 1.HF006	 10260861	
Lucky Count (Bonus Link)	 1.HF008	 10160858	
Jungle Joe Searching High and Low (Bonus Link)	 1.HF009	 10260912	
Fire Light - Power Pay (Bonus Link)	 1.HF010	 10160943	
Fortune Princess (Bonus Link)	 1.HF011	 10160753	
Dolphin Magic - Power Pay (Bonus Link)	 1.HF012	 10160944	
Sirena’s Gold (Bonus Link)	 1.HF013	 10160945	
Crusader’s Heart – Power Pay (Bonus Link)	 1.HF014	 10260856	
5 Dragons (Fa Fa Fa)	 1.HF005	 10160917	
Specific Approval Conditions
1.	The Acres Doli Protocol functionality is not a subject of this approval. 
2.	The number of Jackpot Levels displayed by the ATA Graphics Server of a selected Mystery Link should match the number of Jackpot Levels configured in the Jackpot Controller. 	
Operational Conditions
1.	The Thin Client ATA Graphics Server must be connected to an approved Standard / Hyperlink / Random Link Progressive Jackpot. 
2.	The Thin Client ATA Graphics Server active external I/O ports must be housed in a security cage fitted with a security seal to prevent connection or removal of data cables. 	
Application Reference Number	01-A1175/S01	

System/Device Name	IGT Systems Club 	
Manufacturer	IGT (Australia) Pty Ltd	
Category	Subsidiary Equipment 	
Specification 	18-SET02	
System Description	Data Gathering, Report Generating, Player Tracking / Bonus Points and Ticket In  Ticket Out Validation	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard 4.18	
System Software Identifier	Version 3.2	
Maximum Number of Connected Gaming Machines per Transaction Server	
300	
System Details	
System Name	eCash Redemption Terminal	
Specification Number 	18.SER01	
Category	Gaming Support Systems	
Submission Standards	NS9.0 + NSW Appendix (dated 23/03/07)	
Technical Standards	NS9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Operational Conditions
1.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine. 
2.	The system is approved for use in a local area network (LAN) configuration only. 
3.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS). The UPS must have sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption. Desirably the system should be equipped with a “Smart” UPS capable of automatically shutting the system down in the case of a power failure. 	
Application Reference Number	18-A1192/S01	

System/Device Name	System 7000	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	Subsidiary Equipment	
Main System Software Identifier	7.2.100.26	
Specification Number	01-SET06
01-SEZ07	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard 4.18	
Device Details:	
Device Name	Sprintquip Cashback Centre (approved NI2010-46)	
System Description	Gaming Machines Printed Ticket Redemption Station	
Category	Subsidiary Equipment	
Specification Number	01-SER00	
Submission Standards	NS9.0 + NSW Appendix (dated 23/03/07)	
Technical Standards	NS9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard 4.18	
Operational Conditions
The subsidiary equipment interface card must be housed in a sealed enclosure, which requires access to the secure area of the Gaming Machine.	
Application Reference Number	01-A1196/S01	

System	IGT Systems Max 	
Manufacturer	IGT (Australia) Pty Ltd	
Category	Subsidiary Equipment	
Specification 	18.SET03	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard 4.18	
System Software Identifier	3.1.0 Service Pack 2J	
System Details:	
System Name	eCash Redemption Terminal (approved NI2008-168)	
System Description	Gaming Machine Printed Redemption Station	
Category	Gaming Support System	
Specification Number	18.SER01	
Submission Standards	NS9.0 + NSW Appendix (dated 23/03/07)	
Technical Standards	NS9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard 4.18	
Specific Approval Conditions
1.	All Xtra Credit systems in the field are to be updated with the latest approved system version and functions within 6 weeks from the date of the Xtra Credit approval. 
2.	Approval is limited to single-venue use only. 
3.	Use of the Xtra Credit facility is subject to the requirements of the Gaming Machine Act 2004 and the Gambling and Racing Control (Code of Practice) Regulation 2002. 	
Operational Conditions
1.	The System must be fitted with a compliance plate.
2.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine.
3.	The “IGT Systems Max” is approved for use in a local area network (LAN) configuration only.
4.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS).  The UPS must have sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption.  Desirably the system should be equipped with a “Smart” UPS capable of automatically shutting the system down in the case of a power failure.	
Application Reference Number	18-A1190/S01	

Updated hyperlink LPJS for the ATA Graphics Server	
System/Device Name
	ATA Graphics Server 
Thin Client ATA Graphics Server	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	Gaming Machine	
Gaming Machine Type	Graphics Server	
Specification Number	01-SES00
01-SES01	
Technical Standards	NSW Jackpot Technical Standards Rev 1.1	
Specific Approval Conditions
1.	The Acres Doli Protocol is not a subject of this approval.
2.	The number of jackpot levels displayed by the ATA Graphics Server of a selected Mystery Link should match the number of jackpot levels configured in the Jackpot Controller.	
Operational Conditions
1.	The ATA Graphics Server or Thin Client ATA Graphics Server must be connected to an approved Standard/Hyperlink/Random Link progressive Jackpot System.
2.	The ATA Graphics Server or Thin Client ATA Graphics Server active external I/O ports must be housed in a security cage fitted with a security seal to prevent connection or removal of data cables.	
Application Reference Number	01-A1195/S01	

Updated Standard LPJS Software 	
System/Device Name	Hyperlink LPJS (Max 504 EGM)	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	PC	
PC Type	Standard Progressive Controller	
Specification Number	01-YA002	
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standards Rev 1.1
TITI Technical Standard V4.18 (section 7.1)	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standards Rev 1.1
TITI Technical Standard V4.18 (section 7.1)	
Controller Firmware	Version 5.05	
Additional Jackpot Themes	Bank Buster Link
Cash express/Money Train Link
Beat the Bandits Link	
Specific Approval Conditions
This Hyperlink LPJS (Max 504 EGM) is approved to operate with hyperlink games that have been approved /authorised with the following Hyperlink Link Progressive  Jackpot System Specification Numbers:
Link Configurations	
Gaming Machine Configurations	

Hyperlink LPJS Specification Numbers	
Setting Ids	
Jackpot Themes	
BCV	
Trigger Constants	

01-YH030	
H0030001-H0030008	
Cash Express / Money Train	
1c	
$275	

01-YH290	
H0290001-H0290008	

$350	

01-YH300	
H0300001-H0300008	

$425	

01-YH310	
H0310001-H0310008	

$500	

01-YH320	
H0320001	
Bank Buster	
1c	
$225.25	

01-YA001	
H0030001-H0030008	
Cash Express / Money Train	
1c	
$275	

H0290001-H0290008	

$350	

H0300001-H0300008	

$425	

H0310001-H0310008	

$500	

H0320001	
Bank Buster	
1c	
$225.25	

Operational Conditions
1.	The ATA Graphics Server (1.SES00) or Thin Client ATA Graphics Server (1.SES01) must be connected to the above-mentioned Hyperlink Link Progressive Jackpot System.
2.	There must be at least one venue overhead display connected to the ATA Graphics Server (1.SES00) or Thin Client ATA Graphics Server (1.SES01) so as to display pool values, the serial number/house number of the winning gaming machine and the jackpot win amounts.	
Application Reference Number	01-A1181/S01	

Monitoring System Software Bugfix	
System/Device Name	System 7000	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	Subsidiary Equipment	
Main System Software Identifier	7.3.0.1	
Specification Number	01-SET06
01-SEZ07	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard 4.18	
The System 7000 is approved to operate with the following cash redemption terminal	
Device Name	Sprintquip Cashback Centre (approved NI2010-46)	
System Description	Gaming Machines Printed Ticket Redemption Station	
Category	Subsidiary Equipment	
Specification Number	01-SER00	
Submission Standards	NS9.0 + NSW Appendix (dated 23/03/07)	
Technical Standards	NS9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard 4.18	
Operational Conditions
The subsidiary equipment interface card must be housed in a sealed enclosure, which requires access to the secure area of the Gaming Machine.	
Application Reference Number	01-A1200/S01	

Updated monitoring system software	
System	IGT Systems Club 	
Manufacturer	IGT (Australia) Pty Ltd	
Category	Subsidiary Equipment	
Specification 	18.SET02	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard 4.18	
System Software Identifier	3.2 Service Pack (SP) 22J	
The IGT Systems Club Version 3.2 Service Pack 2 is approved to operate with the following approved cash redemption terminal	
System Name	eCash Redemption Terminal (approved NI2008-168)	
System Description	Gaming Machine Printed Redemption Station	
Category	Gaming Support System	
Specification Number	18.SER01	
Submission Standards	NS9.0 + NSW Appendix (dated 23/03/07)	
Technical Standards	NS9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard 4.18	
Operational Conditions
1.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine. 
2.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS).  The UPS must have sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption.  Desirably the system should be equipped with a “Smart” UPS capable of automatically shutting the system down in the case of a power failure.	
Application Reference Number	18-A1199/S01	

Monitoring System Software Bugfix	
System	IGT Systems Max 	
Manufacturer	IGT (Australia) Pty Ltd	
Category	Subsidiary Equipment	
Specification 	18.SET03	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard 4.18	
Submission Standards	NS 10.0 + NSW Appendix dated (14/01/09)	
System Software Identifier	3.2	
The IGT Systems Club Version 3.2 is approved to operate with the following approved cash redemption terminal	
System Name	eCash Redemption Terminal (approved NI2008-168)	
System Description	Gaming Machine Printed Redemption Station	
Category	Gaming Support System	
Specification Number	18.SER01	
Submission Standards	NS9.0 + NSW Appendix (dated 23/03/07)	
Technical Standards	NS9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard 4.18	
Specific Approval Conditions
1.	Approval is limited to single-venue use only. 
2.	Use of the Xtra Credit facility is subject to the requirements of the Gaming Machine Act 2004 and the Gambling and Racing Control (Code of Practice) Regulation 2002. 	
Operational Conditions 
1.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine. 
2.	The “IGT Systems Max” is approved for use in a local area network (LAN) configuration only. 
3.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS).  The UPS must have sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption.  Desirably the system should be equipped with a “Smart” UPS capable of automatically shutting the system down in the case of a power failure.	
Application Reference Number	18-A1204/S01	

System/Device Name	eBet Netcash CCCE SQL 	
Manufacturer	eBet Gaming Systems Pty Ltd	
Category	Gaming Support system	
Description	Data Gathering, Report Generation, Player Tracking / promotional and Ticket In Ticket Out 	
Specification 	50.SET02	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2 TITO Technical Standard 4.18
NSW Jackpot Technical Standards Rev 1.1	
Operational Conditions
1.	The computer hosting the eBet CCCE SQL system must be physically bolted down in a secure area of the gaming venue with access only permitted to authorised venue personnel.
2.	The system must be installed on a “locked down” computer with a provision for a seal, where no external access devices that are capable of introducing new software or data are accessible on the system without breaking the seal.  This allows access devices such as CDROM drives to facilitate upgrades etc.  However, access to the drive without breaking the seal must be prevented.  This may be achieved by the use of locking sealable faceplates over the drives.
3.	The System, Windows 2000 operating system and MS SQL Server 2000 must be configured so that only the system application and related programs are executable on start-up.
4.	Only those applications that are core to the system operation, and evaluated by GMTF and approved by the Authority are permitted to be configured on a production system.
5.	Any software tool which permits viewing/modification of the data that holds details of audit information must not be installed in the system and neither shall it be in the possession of any eBet employee, or agent, attending service calls.
6.	No editor, compilers, assemblers, or debugging programs are permitted on the system.
7.	There must be no access available to Microsoft Windows Explorer or any other file system tool.
8.	Network facilities on the host system must be restricted to the provision of a network connection to the backup system and associated applications (such as entrance and cashier terminals).  No “dial in” facility is permitted.
9.	The system must be configured in such a way that only authorised personnel have access to critical functions or parameter setting and sensitive information contained in the system.
10.	The system must be installed in a separate discrete network.
11.	The system must be provided and operated with a dedicated Uninterruptible Power Supply (UPS).  The UPS must provide sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption.
12.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine.
13.	The system must be configured with an automated backup facility.
14.	The system’s printer must be operational at all times the system is operating.	

The eBet Netcash CCE SQL is approved to operate with the following approved Cash Redemption terminal:
Device Name:                        Sprintquip Cashback Centre
Specification Number:          50.SER00	
The system is approved to operate in a dual port environment with the following linked progressive jackpot systems that support jackpot CCCE transfer capability:
1.	Any approved Paltronics branded linked progressive jackpot systems;
2.	Any approved Mikhon linked progressive jackpot systems; and
3.	Any Independent Gaming linked progressive jackpot systems version AU0021AR or above.	
Application Reference Number	50.A0093/S01	

Standard Linked Progressive Jackpot System Software Bugfix	
System/Device Name	Standard LPJS 	
Manufacturer	IGT (Australia) Pty Ltd	
Category	Progressive Controller	
Category Type	Standard Progressive Controller	
Specification 	18.YA0008	
Submission Standards
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standards Rev 1.1	
Software Details	
System Firmware	Jackpot Controller (Paltronics): (LJPC2038)	
Firmware ID	OLJ-02-00-03-08-O
OLJ-02-00-03-08-E	
Specific Approval Conditions
The jackpot controller settings listed below are not a subject of this approval and must not be configured in any authorised Standard Link Progressive Jackpot System:
Setting ID: WG006001 – (1c)
Setting ID: WG007001 – (1c)
Setting ID: WG006002 – (2c)
Setting ID: WG007002 – (2c)	
Operational Conditions
1.	The Paltronics Controller and Subsidiary Equipment Interface Card with specified firmware must operate as part of the IGT Standard Linked Progressive Jackpot System with the “Wheel of Fortune” jackpot theme.
2.	The above-mentioned Jackpot Controller / SEI firmware must operate in conjunction with a “Wheel of Fortune” game/shell combination.
3.	When using an overhead display with the VGA Display Driver, the following conditions must be complied with:
a.	The system is to run only under Windows XP operating system;
b.	The keyboard and mouse is to be attached only when performing maintenance and must be removed at all other times;
c.	The PC housing must have a provision to seal all points where the controller cable may be disconnected; and
d.	The write filter application must be loaded on the hard drive set up.
4.	The system interface card must be enclosed in a sealed enclosure.	
Application Reference Number	18.A1206/S01	

Additional Random LPJS Controller for the ATA Graphics Servers	
System/Device Name
	ATA Graphics Server 
Thin Client ATA Graphics Server	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	Gaming Machine	
Gaming Machine Type	Graphics Server	
Specification Number	01-SES00
01-SES01	
Technical Standards	NSW Jackpot Technical Standards Rev 1.1	
LPJS details – 1: Random	
LPJS Type	Software Version	Specification No.	
Paltronics LPJS	XSE01166O/XSE0116E	52.YC001	
	OLJ-02-00-02-01O/OLJ-02-00-02-01E	52.YC001	
Specific Approval Conditions
1.	The Acres Doli Protocol is not a subject of this approval.
2.	The number of jackpot levels displayed by the ATA Graphics Server of a selected Mystery Link should match the number of jackpot levels configured in the Jackpot Controller.	
Operational Conditions
1.	The ATA Graphics Server or Thin Client ATA Graphics Server must be connected to an approved Standard/Hyperlink/Random Link progressive Jackpot System.
2.	The ATA Graphics Server or Thin Client ATA Graphics Server active external I/O ports must be housed in a security cage fitted with a security seal to prevent connection or removal of data cables.	
Application Reference Number	01-A1182/S01	

Monitoring System Gaming Machine Interface Card ‘MCI’ Software Update	
System/Device Name	MCI	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	Subsidiary Equipment	
Category Type	Subsidiary Equipment Interface	
Technical Standards	NSW CPTS Rev 2.2, TITO Technical Standard V4.18	
Software Details	
Description	MCI 224	
Software ID	MCIXC224.BIN	
The following approved system is approved to operate with the above-identified subsidiary equipment interface card ‘MCI Version 2.24’. 	
System Details	
System Name	System 7000	
Specification Number	01-SET06 
01-SEZ07	
System software version	7.3.0.1 and above	
Application Reference Number	01-A1202/S01	

Monitoring System Gaming Machine Interface Card ‘PMM Mk 6’ Software Update	
System/Device Name	PMM Mk 6	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	Subsidiary Equipment	
Category Type	Subsidiary Equipment Interface	
Technical Standards	NSW CPTS Rev 2.2, TITO Technical Standard V4.18	
Software Details	
Device	PMM Mk 6	
Software ID	P6_AN_LABX_116pof
Epcs_controller.flash	
The following approved system is approved to operate with the above-identified subsidiary equipment interface card ‘MCI Version 2.24’. 	
System Details	
System Name	System 7000	
Specification Number	01-SET06 
01-SEZ07	
System software version	7.3.0.1 and above	
Application Reference Number	01-A1203/S01	

Monitoring System Gaming Machine Interface Card ‘Prime Impact’ Software Update	
System/Device Name	Prime Impact	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	Subsidiary Equipment	
Category Type	Subsidiary Equipment Interface	
Technical Standards	NSW CPTS Rev 2.2, TITO Technical Standard V4.18	
Software Details	
Description	PRIME Impact	
Software ID	Sentinel3.exe	
The following approved system is approved to operate with the above-identified subsidiary equipment interface card ‘MCI Version 2.24’. 	
System Details	
System Name	System 7000	
Specification Number	01-SET06 
01-SEZ07	
System software version	7.3.0.1 and above	
Application Reference Number	01-A1201/S01	

IGT systems club software updates with Xtra Credit 	
System 1	IGT Systems Club 	
Manufacturer	IGT (Australia) Pty Ltd	
Category	Subsidiary Equipment	
Specification 	18.SET02	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard 4.18	
System 2	IGT Systems Club  remote Site	
Manufacturer	IGT (Australia) Pty Ltd	
Category	Subsidiary Equipment	
Specification 	18.SET04	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard 4.18	
System Software Identifier	3.4	
The IGT Systems Club Version 3.4 is approved to operate with the following approved cash redemption terminal	
System Name	eCash Redemption Terminal (approved NI2008-168)	
System Description	Gaming Machine Printed Redemption Station	
Category	Gaming Support System	
Specification Number	18.SER01	
Submission Standards	NS9.0 + NSW Appendix (dated 23/03/07)	
Technical Standards	NS9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard 4.18	
Specific Approval Conditions
1.	Use of the Xtra Credit facility is subject to the requirements of the Gaming Machine Act 2004 and Gambling and Racing Control (Code of Practice) Regulation 2002.
2.	The Xtra Credit functionality is limited to single venue use only.	
Operational Conditions
1.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine. 
2.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS).  The UPS must have sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption.  Desirably the system should be equipped with a “Smart” UPS capable of automatically shutting the system down in the case of a power failure.	
Application Reference Number	18-A1205/S01, / S02	

Updated Jackpot Display Controller for previously approved Standard LPJS and regression tested games	
System/Device Name	Standard LPJS-Mystical Temple	
Manufacturer	Konami Australia Pty Ltd	
Category	Progressive Controller	
Category Type	Standard Progressive Controller	
Specification 	39.YA002	
Submission Standards
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standards Rev 1.1	
Jackpot Theme	Mystical Temple	
List of previously approved games for operation with the above-mentioned Standard LPJS and the updated Jackpot Display Controller	
Game Name	Specification Number	Program ID	
Gold and Ruins Mystical Temple	39.H0043	GAR7NC10	
Relic Hunting Mystical Temple	39.H0044	REL7NB10	
Jungle Jewel Mystical Temple	39.H0045	JUN7NC10	
Incan Spirit Mystical Temple	39.H0046	INS7NA10	
Operational Conditions
The system interface card must be enclosed in a sealed enclosure.	
Application Reference Number	39-A0893/S01	

New Standard Linked Progressive Jackpot System 	
System Name	Standard LPJS	
Manufacturer	Ainsworth Game Technology Ltd (AGT)	
Category	Progressive Controller	
Category Type	Standard Progressive Controller	
Specification 	44.YA005	
Submission Standards
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standards Rev 1.1	
Controller Firmware	Version 02.00.03.02	
Interface Card Firmware	Version 1.27	
Jackpot Theme	Classic	
Operational Conditions
1.	The Paltronics Controller and Subsidiary Equipment Interface Card with specified firmware must operate as part of AGT’s Standard Linked Progressive Jackpot System with the ‘Classic’ game theme.
2.	The above-mentioned Jackpot Controller / SEI firmware must operate in conjunction with a ‘Classic’ game / shell combination. 
3.	The system interface card must be enclosed in a sealed enclosure.	
Application Reference Number	44-A0615/S01	

Updated Standard Linked Progressive Jackpot System 	
System Name	Standard LPJS	
Manufacturer	Ainsworth Game Technology Ltd (AGT)	
Category	Progressive Controller	
Category Type	Standard Progressive Controller	
Specification 	44.YA005	
Submission Standards
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standards Rev 1.1	
Controller Firmware	Version 02.00.03.02	
Interface Card Firmware	Version 1.27	
Jackpot Theme	Rio Grande Rapids	
Operational Conditions
1.	The Paltronics Controller and Subsidiary Equipment Interface Card with specified firmware must operate as part of AGT’s Standard Linked Progressive Jackpot System with the ‘Rio Grande Rapids’ game theme.
2.	The above-mentioned Jackpot Controller / SEI firmware must operate in conjunction with a ‘Rio Grande Rapids’’ game / shell combination. 
3.	The system interface card must be enclosed in a sealed enclosure.	
Application Reference Number	44-A0604/S01