Australian Capital Territory
Gaming Machine (Peripheral Equipment) Approval 2014 (No 9)
Notifiable instrument NI2014– 435
made under the  
Gaming Machine Act 2004, section 69 (Approval of gaming machines and peripheral equipment)

1	Name of instrument
This instrument is the Gaming Machine (Peripheral Equipment) Approval 2014 (No 9).

2	Commencement 
This instrument commences on the day after its notification.

3	Approval
I approve the peripheral equipment described in the attached Schedule to this instrument.  

4	Revocation
This instrument revokes:

•	NI2011-5	•	NI2011-220	•	NI2011-585	
•	NI2011-22	•	NI2011-248	•	NI2011-617	
•	NI2011-33	•	NI2011-276	•	NI2011-646	
•	NI2011-40	•	NI2011-277	•	NI2011-717	
•	NI2011-114	•	NI2011-278	•	NI2011-791	
•	NI2011-150	•	NI2011-454	•	NI2011-803	
•	NI2011-216	•	NI2011-540		

James Mullan
Delegate
ACT Gambling and Racing Commission

28 August 2014

Standard Linked Progressive System Software Bugfix 	
System/Device Name	Standard LPJS – Jackpot Jewels	
Manufacturer	IGT (Australia) Pty Ltd	
Category Type	Progressive Controller	
Progressive Controller Type	Standard Progressive Controller	
Specification 	18.YA008	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standards Rev 1.1	
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standards Rev 1.1	
LPJS Description	1 level Standard Linked Progressive Jackpot Controller and Interface Card with CCCE Port Sharing Functionality	
Controller Firmware	Version 02.00.03.08	
Interface Card Firmware	Version 1.21	
Operational Conditions
1.	The Paltronics Controller and Subsidiary Equipment Interface Card with specified firmware must operate as part of the IGT Standard Linked Progressive Jackpot System with the “Jackpot Jewels” jackpot theme.
2.	The above-mentioned Jackpot Controller/SEI firmware must operate in conjunction with a “Jackpot Jewels” game/shell combination.
3.	An overhead display must be used as part of the LPJS.
4.	When using an overhead display with the VGA Display Driver, the following conditions must be complied with:
a)	The system is to run only under Windows XP operating system.
b)	The keyboard and mouse is to be attached only when performing maintenance and must be removed at all other times.
c)	The PC housing must have a provision to seal all points where the controller cable may be disconnected.
d)	The write filter application must be loaded on the hard drive set up.
5.	The system interface card must be enclosed in a sealed enclosure.	
Application Reference Number	18.A1207/S01	

Updated Hardware Assemblies	
System/Device Name	Coin Validator	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Category	Gaming Machine	
Gaming Machine Type	Hardware Component	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Hardware Details	
Condor Premium Coin Validator:	Part Number: C2130SAU00005
Manufacturer: Money Controls	
Platform/Cabinet	GENEX – Midway, Lowboy, G-Deluxe	
Application Reference Number	06-A0300/S01; 06-A0301/S01	

Updated Hardware Assemblies	
System/Device Name	Power Supply Unit	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Category	Gaming Machine	
Gaming Machine Type	Hardware Component	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Hardware Details	
Power Supply Unit:	Model: EDPS-350DB A
Manufacturer: Delta Electronics Inc. 	
Platform/Cabinet	GENEX – Midway, Lowboy, G-Deluxe	
Application Reference Number	06-A0300/S01; 06-A0301/S01	

Updated Standard LPJS Software 	
System/Device Name	Hyperlink LPJS (Max 504 EGM)	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	PC	
PC Type	Standard Progressive Controller	
Specification Number	1.YA002 (SLPJS)
1.SES00 (ATA Graphics Server)
1.SES01 (Thin Client ATA graphics Server)	
Technical Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standards Rev 1.1
TITI Technical Standard V4.18 (section 7.1)	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standards Rev 1.1
TITI Technical Standard V4.18 (section 7.1)	
Controller Firmware	Version 6.00	
Interface Card Firmware	Version 11.0	
Specific Approval Conditions
This Hyperlink LPJS (Max 504 EGM) is approved to operate with hyperlink games that have been approved /authorised with the following Hyperlink Link Progressive  Jackpot System Specification Numbers:
Link Configurations	
Gaming Machine Configurations	

Hyperlink LPJS Specification Numbers	
Setting Ids	
Jackpot Themes	
BCV	
Trigger Constants	

01-YH030	
H0030001-H0030008	
Cash Express / Money Train	
1c	
$275	

01-YH290	
H0290001-H0290008	

$350	

01-YH300	
H0300001-H0300008	

$425	

01-YH310	
H0310001-H0310008	

$500	

01-YH320	
H0320001	
Bank Buster	
1c	
$225.25	

01-YA001	
H0030001-H0030008	
Cash Express / Money Train	
1c	
$275	

H0290001-H0290008	

$350	

H0300001-H0300008	

$425	

H0310001-H0310008	

$500	

H0320001	
Bank Buster	
1c	
$225.25	

Operational Conditions
1.	The ATA Graphics Server (1.SES00) or Thin Client ATA Graphics Server (1.SES01) must be connected to the above-mentioned Hyperlink Link Progressive Jackpot System.
2.	There must be at least one venue overhead display connected to the ATA Graphics Server (1.SES00) or Thin Client ATA Graphics Server (1.SES01) so as to display pool values, the serial number/house number of the winning gaming machine and the jackpot win amounts.	
Application Reference Number	01-A1213/S01	

Monitoring System Interface Card Software Bugfix	
System/Device Name	Interface Card	
Manufacturer	IGT (Australia) Pty Ltd	
Category	Subsidiary Equipment	
Category Type	Subsidiary Equipment Interface Card	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard V4.18 	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Software Details	
Device Name	File name	Version	
Interface Card – iBoard	iBoard.jar#	130295	
Display Board – sbNexGen	Overton.exe	2.01.08-SP2	
The interface card software “iBoard version 130295” and Overton version 2.01.08 Sp2” are approved to operate with the following approved systems.	
System Details 1	
System Name 	IGT Systems Club	
Specification Number	18.SET02	
System Software Version	3.4	
System Details 2	
System Name 	IGT Systems Club – Remote Site	
Specification Number	18.SET04	
System Software Version	3.4	
System Details 3	
System Name 	IGT Systems Max	
Specification Number	18.SET03	
System Software Version	3.2, 3.2T	
Retrofit Order
A retrofit of all effected devices in the field in ACT with the abovementioned interface card software is required to retrofit the previously approved software version “iBoard version 130293, 1302089” and ”Overton version 2.01.07 SP2, 2.01.03 SP2”.	
Operational Conditions
The interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine.	
Application Reference Number	18-A1213/S01, 18-A1214/S01	

Monitoring System Machine Communication Interface “MCI” Software Bugfix	
Device Name	MCI (Machine Communication Interface)	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	SE (Subsidiary Equipment)	
Gaming Machine Type	SEI (Subsidiary Equipment Interface Card)	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS Rev 2.2
TITO Technical Standard Version 4.18	
Software Details	
Device	Software ID	Device Type	Pos	Ver.	CRC32	
MCI 225	MCIXC225.BIN	EPROM	U4	2.25	C694EF55	
The above identified MCI version 2.25 is approved to operate with the following approved monitoring system:	
System Name	SYSTEM 7000	
Category	SE (Subsidiary Equipment)	
Specification Number	01-SET06 & 01-SEZ07	
System Software Identifier	7.2.100.26 and above	
Submission Standards	NS 10.0 + NSW Appendix dated 14/01/09	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard Version 4.18 	
Operational Conditions
1.	The machine communication interface card must be housed in a sealed enclosure, which requires access to the secure area of the Gaming Machine.	
Application Reference Number	01-A1228/S01	

Monitoring System “System 7000” Software Bugfix	
System Details 1	SYSTEM 7000	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	SF (Supporting Function)	
Specification Number	01-SET06 & 01-SEZ07	
System Software Identifier	7.3.0.1	
Submission Standards	NS 10.0 + NSW Appendix dated 14/01/09	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard V4.18 	
Software Details 1	
File Name	System 7000 Floor Server Description	Version	CRC 32	
Dacom Install	Dacom-install-5.31.tar	5.31	c098e5e8	
Install Dacom	Install-dacom-5.31.zip	5.31	f062f4fc	
Master	Master-5.31.zip	5.31	6b9f00cd	
System Details 2	
System Name 	SYSTEM 7000	
Category	SF (Supporting Function)	
Specification Number	01-SET06 & 01-SEZ07	
System Software Identifier	7.2.100.26	
Submission Standards	NS 10.0 + NSW Appendix dated 14/01/09	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard V4.18 	
Software Details 2				
File Name	System 7000 Floor Server Description	Version	CRC 32	
Dacom Install	Dacom-install-5.23.tar	5.23	D1169DFD	
Install Dacom	Install-dacom.zip	5.23	B737188D	
Master	Master-5.23.zip	5.23	4F7A9489	
Application Reference Number	01-A1227/S01	

Standard Linked Progressive Jackpot System Jackpot Parameter Update	
System Name	Standard LPJS	
Manufacturer	IGT (Australia) Pty Ltd	
Category	PC (Progressive Controller)	
PC Type	STD (Standard Progressive Controller)	
Specification Number	18.YA008	
LPJS Description	4 level Standard Linked Progressive Jackpot Controller and Interface Card with CCCE Port Sharing Functionality	
Technical Standards
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standards Rev 1.1	
Controller Firmware	Version 3.08	
Interface Card Firmware	Version 1.21	
Jackpot Themes	Wheel of Gold	
Operational Conditions
1.	The Paltronics Controller and Subsidiary Equipment Interface Card with specified firmware must operate as part of the IGT Standard Linked Progressive Jackpot System with the “Wheel of Gold” jackpot theme.
2.	The above-mentioned Jackpot Controller / SEI firmware must operate in conjunction with the “Wheel of Gold” game / shell combination.
3.	When using an overhead display with the VGA Display Driver, the following conditions must be complied:
a)	The system is to be run only under Windows XP operating system.
b)	The keyboard and mouse is to be attached only when performing maintenance and must be removed at all other times.
c)	The PC housing must have a provision to seal all points where the controller cables may be disconnected.
d)	The write filter application must be loaded on the hard drive at start up.
4.	The system interface card must be enclosed in a sealed enclosure.	
Application Reference Number	18-A1215/S01	

Updated Standard Linked Progressive Jackpot System	
System Name	Standard LPJS	
Manufacturer	Ainsworth Game Technology Limited	
Category	PC (Progressive Controller)	
PC Type	STD (Standard Progressive Controller)	
Specification Number	44.YA005	
LPJS Description	Standard Linked Progressive Jackpot Controller and Interface Card with CCCE Port Sharing Functionality	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standards Rev 1.1	
Controller Firmware	Version 02.00.03.08	
Interface Card Firmware	Version 1.44	
Jackpot Themes	a) Classic
b) Rio Grande Rapids
c) Players Paradise	
Previously approved games suitable for operation with the Players Paradise LPJS	
Game Name	Spec. Number	Program ID	
Vegas Fantasy (BCV 1c)	44.HF051	GANSVS1D	
Vegas Fantasy (BCV 2c)	44.HF052	GANSVS2D	
Vegas Fantasy (BCV 5c)	44.HF053	GANSVS3D	
Vegas Fever (BCV 1c)	44.HF054	GANSVV1E	
Vegas Fever (BCV 2c)	44.HF055	GANSVV2E	
Vegas Fever (BCV 5c)	44.HF056	GANSVV3E	
Vegas Fortune (BCV 1c)	44.HF057	GANSVF1E	
Vegas Fortune (BCV 2c)	44.HF058	GANSVF2E	
Vegas Fortune (BCV 5c)	44.HF059	GANSVF3E	
Vegas Frenzy (BCV 1c)	44.HF060	GANSVZ1C	
Vegas Frenzy (BCV 2c)	44.HF061	GANSVZ2C	
Vegas Frenzy (BCV 5c)	44.HF062	GANSVZ3C	
Vegas Fantasy (BCV 1c)	44.HF063	GDNSVS1D	
Vegas Fantasy (BCV 2c)	44.HF064	GDNSVS2D	
Vegas Fantasy (BCV 5c)	44.HF065	GDNSVS3D	
Vegas Fever (BCV 1c)	44.HF066	GDNSVV1D	
Vegas Fever (BCV 2c)	44.HF067	GDNSVV2D	
Vegas Fever (BCV 5c)	44.HF068	GDNSVV3D	
Vegas Fortune (BCV 1c)	44.HF069	GDNSVF1D	
Vegas Fortune (BCV 2c)	44.HF070	GDNSVF2D	
Vegas Fortune (BCV 5c)	44.HF071	GDNSVF3D	
Vegas Frenzy (BCV 1c)	44.HF072	GDNSVZ1C	
Vegas Frenzy (BCV 2c)	44.HF073	GDNSVZ2C	
Vegas Frenzy (BCV 5c)	44.HF074	GDNSVZ3C	
Vegas Fiesta (BCV 1c)	44.HF085	GANSVA1B	
Vegas Fiesta (BCV 2c)	44.HF086	GANSVA2B	
Vegas Fiesta (BCV 5c)	44.HF087	GANSVA3B	

Continued
Operational Conditions
1.	The Paltronics Controller and Subsidiary Equipment Interface Card with specified firmware must operate as part of the AGT’s Standard Linked Progressive Jackpot System with the ‘Classic’ / ‘Rio Grande Rapids’ / ‘Players Paradise’ game theme.
2.	The above-mentioned Jackpot Controller / SEI firmware must operate in conjunction with the ‘Classic’ / ‘Rio Grande Rapids’ / ‘Players Paradise’ game / shell combination.
3.	The system interface card must be enclosed in a sealed enclosure.	
Application Reference Number	44-A0621/S01	

Updated Bill Acceptor Firmware	
System/Device Name	Bill Acceptor	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	GM (Gaming Machine)	
Category Type	Other (BNA Firmware)	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standards Rev 1.1	
Bill Acceptor Details	MEI Cashflow SC Series – SC6607
ATA P/N: 579125_12 – Gen7 Viridian / Gen7
Viridian Widescreen
ATA P/N:578471_12 – Gen7 Slant
ATA P/N: 578447_12 – Gen7 Upgrade	
Platform/Cabinet Details	Gen7 Viridian – Chop Top, Casino Top
(with in-machine LCD) (Configured with either Ticket Printer and/or Hopper option)
Gen7 Slant – Round Top, Casino Top (with in-machine LCD) (Configured with Ticket Printer only)
Gen7 Upgrade XCite – Lowboy (Configured with either Ticket Printer and/or Hopper option)
Gen7 Upgrade Xtreme - Casino Top (with in-machine LCD) (Configured with either Ticket Printer and/or Hopper option)
Gen7 Viridian Widescreen - Chop Top, Casino Top (with in-machine LCD) (Configured with either Ticket Printer and/or Hopper option)	
Application Reference Number	01-A1226/S01	

Monitoring System Subsidiary Equipment Interface “Prime Impact” Software Bugfix	
System/Device Name	Prime Impact	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	SE (Subsidiary Equipment)	
Category Type	SEI (Subsidiary Equipment Interface Card)	
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard 4.18	
Software Details	
Description	Software ID	Type	Ver.	CRC 32	HMAS SHA1	
PRIME Impact	Sentinel3.exe	CF	2.01	4E35f39E	7fc3d994 b6a36290 b73d9cb3 e6b2d1f6 0c891549	
BIOS	S3boot107.bin	EPROM	1.07	7654D1CB	B0F183DA 59A89E28 66514012 E4989737 0913C3AB	
Operating System	MS Windows CE 5.0					
The above identified Prime Impact version 2.01 is approved to operated with the following approved monitoring system:	
System Details	
System Name	System 7000	
Category	SE (Subsidiary Equipment)	
Specification Number	01-SET06 & 01- SEZ07	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard 4.18	
System Software Identifier	7.2.100.26 and above	
Operational Conditions
1.	The subsidiary equipment interface card must be housed in sealed enclosure, which requires access to the secure area of the Gaming Machine.	
Application Reference Number	01-A1229/S01	

Bill Acceptor Firmware Update	
System/Device Name	Bill Acceptor	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Category	GM (Gaming Machine)	
Category Type	Hardware Component (Bill Acceptor)	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Hardware Details	MEI SC66 Bill Acceptor P/N: CFSC66
Bill Acceptor Enclosure P/N: CEK030500
Wiring P/N: 3EK043600-G	
Platform/Cabinet Details	GENEX – Midway, Lowboy, G-Deluxe	
Application Reference Number	06-A0306/S01	

Alternate Power Supply Units	
System/Device Name	Power Supply Unit	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Category	GM (Gaming Machine)	
Category Type	Hardware Component	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
	
Hardware Details 1	
Power Supply Unit	Model: LPS-75-24
Manufacturer: Mean Well Enterprises Co. Ltd.	
Platform / Cabinet Details	GENEX – Midway, Lowboy, G-Deluxe	
Hardware Details 2	
Power Supply Unit	Model: LPS-75-5 & LPS-75-12
Manufacturer: Mean Well Enterprises Co. Ltd.	
Platform / Cabinet Details	GENEX – G-Deluxe	
Application Reference Number	06-A0303/S01	

Alternate Peripheral Device	
System/Device Name	Banknote Acceptor	
Manufacturer	Konami Australia Pty Ltd	
Category	GM (Gaming Machine)	
GM Type	Hardware Component	
Technical Standards

	NS 9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Submission Standards	NS 9.0 + NSW Appendix (dated 23/03/07)	
Banknote Acceptor ID	CashCode Model FLS2310
Konami Part Number: 508 CAS	
Software Details	
Description	Firmware Ver	Memory Card Program ID	CashCode Reader CRC	HMAC-SHA1	
Banknote Acceptor Firmware	F(AUS)-85; ID003-04V2220804	FLS-AU22-220804	3C4A	aceed5c6 a2c0f72f 4b6ea20f 784b0646 e473b763	
Hardware Details	
Description	Part Number	
Stacker:	Konami P/N: 5082007A
(AU$, 600 notes)	
Validating Head + Bezel:	Konami P/N: 5082006A	
Platform/Cabinet Details
	Endeavour Series – High Top, Low Boy, Casino Top, Casino Top with LPJS
ES 500 – Low Boy, Casino Top, Casino Top with LPJS
K2V – Casino Top, Low Boy, Casino Top with LCD
K2V 500 – Casino Top, Low Boy, Casino Top with LCD
K2V Upgrade – Casino Top, Low Boy
K2V 500 Upgrade – Casino Top, Low Boy	
Application Reference No.	39-A0779/S01	

Alternate Peripheral Device	
System/Device Name	Thermal Ticket Printer	
Manufacturer	Konami Australia Pty Ltd	
Category	GM (Gaming Machine)	
GM Type	Hardware Component	
Technical Standards

	NS 9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Submission Standards	NS 9.0 + NSW Appendix (dated 23/03/07)	
Ticket Printer ID	Nanoptix Model PayCheck 3
Konami Part Number: 310201A	
Software Details	
Description	Firmware Ver	Flash ROM Program ID	HMAC-SHA1	
Ticket Printer Firmware	PAY-3.63K	Paycheck3_V3_63K	829f6589 47460d95 93b4c302 a411b03d 55256565	
Platform/Cabinet Details
	Endeavour Series – High Top, Low Boy, Casino Top, Casino Top with LPJS
ES 500 – Low Boy, Casino Top, Casino Top with LPJS
K2V – Casino Top, Low Boy, Casino Top with LCD
K2V 500 – Casino Top, Low Boy, Casino Top with LCD
K2V Upgrade – Casino Top, Low Boy
K2V 500 Upgrade – Casino Top, Low Boy	
Application Reference No.	39-A0779/S01	

Previously Approved LCD Display Software for a new Random LPJS	
System/Device Name	LCD Display (Random LPJS)	
Manufacturer	Konami Australia Pty Ltd	
Category	SF (Supporting Function)	
SF Type	Other (LCD Display Software)	
Technical Standards
Submission Standards	NS 8.0 + NSW Appendix (dated 28/04/05)	
Software Details	
Firmware	EPROM Label	Position	HMAC-SHA1	
LCD EPROM	2DP3NA01.ROM1	MMB (ROM1) / MPU(Slave)	b9e2450e ed30edbb 4a6a19bd d986fba5 f35b0d37	
LCD EPROM	2DP3NA01.ROM2	MMB (ROM2) / MPU(Slave)	a4ca27e8 4f5439ee e53cf6ae a6f4548a 29139978	
LCD Graphics Flash ID	2DP3001C.CF	MPU(Slave)	2991fd16 af15816d 64f2eb41 4ee9e0d9 230560ca	
Hardware Details	
Description	Part Number	
Secondary MPU Board (Slave):	PWB (B4) 0000292786	
Secondary MPU Board (Slave) RoHS:	PWB (B5) 0000292786	
Secondary Memory Board (MMB):	PWB (C1) 0000295351	
SEI to MPU (Slave) Cable:	821-6127	
Platform/Cabinet Details	KGP 2.0 UVS - Podium	
Previously Approved Games for use with this LCD Firmware	
Game Details 1	
Game Name	Eternal Gold	
Specification Number	39.A0275	
Category	GM (Gaming Machine)	
GM Type	Conventional	
Game Type	Spinning Reels	
Technical Standards

	NS 9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Submission Standards	NS 9.0 + NSW Appendix (dated 23/03/07)	
Platform/Cabinet Details	K2V – Casino Top, Low Boy, Casino Top with LCD
K2V Upgrade – Casino Top, Low Boy
K2V 500 – Casino Top, Low Boy, Casino Top with LCD
K2V 500 Upgrade – Casino Top, Low Boy
KGP 2.0 UVS - Podium	

Continued
Game Details 2	
Game Name	Treasure Voyage	
Specification Number	39.A0278	
Category	GM (Gaming Machine)	
GM Type	Conventional	
Game Type	Spinning Reels	
Technical Standards

	NS 9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Submission Standards	NS 9.0 + NSW Appendix (dated 23/03/07)	
Platform/Cabinet Details	K2V – Casino Top, Low Boy, Casino Top with LCD
K2V Upgrade – Casino Top, Low Boy
K2V 500 – Casino Top, Low Boy, Casino Top with LCD
K2V 500 Upgrade – Casino Top, Low Boy
KGP 2.0 UVS - Podium	
Operational Conditions
1.	The KGP 2.0 UVS platform with the ‘Money Dragon’ LPJS LCD Display software installed in the Top Display Controller, must be used in conjunction with the Paltronics Random Link Progressive Jackpot System, Specification Number 52-YCKA0, firmware version 1.05 and the Paltronics Interface (SEI) firmware version 1.02, configured as a 2 level mystery jackpot.	
Application Reference No.	39-A0802/S01	

Updated VGA Display Driver Details For Previously Approved Standard Linked Progressive Jackpot System	
System/Device Name	Standard LPJS	
Manufacturer	Ainsworth Game Technology Limited	
Category	PC (Progressive Controller)	
PC Type	STD (Standard Progressive Controller)	
Specification Number	44.YA005	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standard Rev 1.1	
Controller Firmware	02.00.03.02	02.00.03.08	
Interface Card Firmware	1.27	1.44	
Jackpot Theme	Rio Grande Rapids	
Operational Conditions
1.	The Paltronics Controller and Subsidiary Equipment Interface Card with specified firmware must operate as part of AGT’s Standard Linked Progressive Jackpot System with the ‘Rio Grande Rapids’ game theme.
2.	The above-mentioned Jackpot Controller / SEI firmware must operate in conjunction with a ‘Rio Grande Rapids’ game / shell combination.
3.	The system interface card must be enclosed in a sealed enclosure.
4.	When using an overhead display with the VGA Display Driver, the following conditions must be complied:
a)	The system is to be run only under Windows XP operating system.
b)	The keyboard and mouse is to be attached only when performing maintenance and must be removed at all other times.
c)	The PC housing must have a provision to seal all points where the controller cables may be disconnected.
d)	The write filter application must be loaded on the hard drive at start up.	
Application Reference Number	44-A0640/S01; 44-A0618/S01	

Updated ATA Graphics Server Hyperlink & Mystery Link Configurations	
Device Name	Gen7 Viridian Widescreen Platform Hyperlink & Mystery Link Configurations (incorporating the ATA Graphics Server)	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	GM (Gaming Machine)	
Category Type	Other (Dealer Display)	
Specification Number	01-SES00
01-SES01	
Submission Standards 
Technical Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2	
Platform/Cabinet Details	
a)	Hyperlink Configuration:	Gen7 Viridian Widescreen – Chop Top (with/without external LCD + overhead VGA display for Hyperlink) (Configured with either Ticket Printer and/or Hopper option)
Gen7 Viridian Widescreen – Casino Top (with in-machine LCD for Hyperlink) (Configured with either Ticket Printer and/or Hopper option)	
b)	Mystery Link Configuration:	Gen7 Viridian Widescreen – Chop Top (with/without external LCD + overhead VGA display for Mystery Link) (Configured with either Ticket Printer and/or Hopper option)
Gen7 Viridian Widescreen – Casino Top (with in-machine LCD for Mystery Link) (Configured with either Ticket Printer and/or Hopper option)	
List of previously approved games recommended for use on the Gen7 Viridian Widescreen Platform Hyperlink Configurations:	
Game Name	Specification Number	Program ID	
Dragon Emperor (Bonus Link)	1.HF023	10161175	
Don Quixote (Bonus Link)	1.HF024	10261183	
Jazee (Bonus Link)	1.HF025	10161173	
List of previously approved games recommended for use on the Gen7 Viridian Widescreen Platform Mystery Link Configurations:	
Game Name	Specification Number	Program ID	
Stuck On You	1.F0068	10161187	
Dragon Emperor	1.F0070	10161174	
Don Quixote	1.F0071	10261193	
The Phantom	1.F0072	10261295	
Jazee	1.F0073	10161172	
2Can	1.F0079	10361190	
Jackpot Catcher	1.BF017	10261250	
Chariot Champion	1.BF018	10261232	

Continued
Specific Approval Conditions
1.	The Acres Doli Protocol functionality is not a subject of this approval.
2.	The display content and access to display parameters must be implemented in a secure manner to prevent unauthorised access.  That is, access is limited to authorised Aristocrat personnel or authorised Aristocrat agents.
3.	The display is not to be used for the purpose of advertising or promotions.
4.	The jackpot pool values are to be displayed to the players generally most of the time (i.e. the display must keep players informed of the current state of the jackpot(s)).
5.	The number of Jackpot Levels displayed by the ATA Graphics Server of a selected Mystery Link should match the number of Jackpot Levels configured in the Jackpot Controller.
6.	The display is not to be used for feature or bonus games.
7.	The display material is not to be offensive and harm minimisation must be considered.	
Operational Conditions
1.	The ATA Graphics Server must be connected to an approved Linked Progressive Jackpot System as given above.
2.	The ATA Graphics Server active external I/O ports must be housed in a security cage fitted with a security seal to prevent connection or removal of data cables.	
Application Reference No.	01-A1205/S01	

Updated Bill Acceptor Firmware	
System/Device Name	Bill Acceptor	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Category	GM (Gaming Machine)	
GM Type	Other (Bill Acceptor Firmware)	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Hardware Details	
MEI SC66 Bill Acceptor:	Part number: CFSC66	
Bill Acceptor Enclosure:	Part number: CEK030500	
Wiring:	Part number: 3EK043600-G	
Firmware Details	
Firmware ID	Firmware File:	HMAC-SHA1	
Application Firmware: 282067310 (V3.10)	282067310_SC66_MEI_APP_FLASH.bin	f4784d74 8c64a9a6 55da9293 93e341bd 7366d51e	
Variant (Bill-Set) Firmware 490339203 (V2.03)	490339203_SC66_AUD
_FLASH.BIN	7eda250e cca33902 11e0da67 75d1e8a1 95d93334	
Platform/Cabinet Details	GENEX – Midway, Lowboy, G-Deluxe	
Application Reference Number	06-A0316/S01	

Updated Bill Acceptor Firmware	
System/Device Name	Bill Acceptor	
Manufacturer	Konami Australia Pty Ltd	
Category	GM (Gaming Machine)	
GM Type	Other (BNA Firmware)	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2	
Bill Acceptor Identification	MEI Cashflow Model SC6607 AS
Konami Part Number: 3082020A	
Software Details	
Description	Firmware Ver	File Name	HMAC-SHA1	
Application Firmware	V3.10, 282067310	282067310_SC66_MEI_APP_FLASH.BIN	7eda250e cca33902 11e0da67 75d1e8a1 95d93334	
Variant (Bill-set) Firmware	V2.03, 490339203	490339203_SC66_AUD_FLASH.BIN	f4784d74 8c64a9a6 55da9293 93e341bd 7366d51e	
Hardware Details		
Description	Part Number	
Stacker:	Konami P/N: 3082021A	
Validating Head:	Konami P/N: 5082013A	
Platform/Cabinet Details	KGP 2.0 UVS Podium – Upper LCD Box, Tombstone LCD Box, Short Top Box	
Operational Conditions
1.	In the EGM Setup Configuration Mode, the MEI Cashflow Bill Acceptor is configured as Mars Bill Acceptor.	
Application Reference Number	39-A0920/S01	

Updated Standard LPJS	
System/Device Name 1	Standard LPJS – Grand Central	
Manufacturer	Shuffle Master Australasia Pty Limited	
Specification Number	35-YA000	
Category	PC (Progressive Controller)	
PC Type	Standard Progressive Controller	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot TS Rev 1.1
TITO Technical Standard V4.18 (Section 7.1)	
Controller Firmware	Version 02.00.03.09	
Interface Card Firmware	Version 1.27	
Jackpot Theme	Train	
List of previously approved games suitable for operation on the above-mentioned LPJS:	
No	Game Name	Spec Number	Program ID	
1	Sycee – Grand Central (BCV 1c)	35-HF000	SGCNSW1E	
2	Sycee – Grand Central (BCV 2c)	35-HF001	SGCNSW1E	
3	Oceanus – Grand Central (BCV 1c)	35-HF002	OGCNSW1D	
4	Oceanus – Grand Central (BCV 2c)	35-HF003	OGCNSW1D	
5	Gold Country – Grand Central (BCV 1c)	35-HF004	GGCNSW1G	
6	Gold Country – Grand Central (BCV 2c)	35-HF005	GGCNSW1G	
7	Lonesome George – Grand Central (BCV 1c)	35.HF010	LGCNSW2A	
8	Lonesome George – Grand Central (BCV 2c)	35.HF011	LGCNSW2A	
9	Lakota – Grand Central (BCV 1c)	35.HF012	KGCNSW1A	
10	Lakota – Grand Central (BCV 2c)	35.HF013	KGCNSW1A	
11	Archipelago Grand Central (BCV 1c)	35.HF014	AGCNSW1B	
12	Archipelago Grand Central (BCV 2c)	35.HF015	AGCNSW1B	
System/Device Name 2	Standard LPJS – Ultimate	
Manufacturer	Shuffle Master Australasia Pty Limited	
Specification Number	35-YA001	
Category	PC (Progressive Controller)	
PC Type	Standard Progressive Controller	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot TS Rev 1.1
TITO Technical Standard V4.18 (Section 7.1)	
Controller Firmware	Version 02.00.03.09	
Interface Card Firmware	Version 1.27	
Jackpot Theme	Ultimate	
List of previously approved games suitable for operation on the above-mentioned LPJS:	
No	Game Name	Spec Number	Program ID	
1	Ultimate Amazonia	35-HF006	UAMNSW1B	
2	Ultimate 1812	35.HF009	U18NSW1C	

Continued
Operational Conditions
1.	The Paltronics Controller and Subsidiary Equipment Interface Card with specified firmware must operate as part of the Stargames Standard Linked Progressive Jackpot System using the ‘Grand Central’ / ‘Ultimate’ game theme.
2.	For the ‘Grand Central’ LPJS, the Paltronics Controller’s Auto-pay flag must be set to 25 seconds or more to ensure complete winning animations on the overhead jackpot display.
3.	When using a display with the VGA Display Driver, the following conditions must be complied:
a)	The system is to be run only under Windows XP operating system.
b)	The keyboard and mouse is to be attached only when performing maintenance and must be removed at all other times.
c)	The PC housing must have a provision for a LAB seal to seal all points where the controller cables may be disconnected.
d)	The write filter application must be loaded on the hard drive at start up.
4.	The system interface card must be enclosed in a sealed enclosure.	
Application Reference Number	35-A0691/S01, /S02	

Standard Linked Progressive Jackpot System Update	
System/Device Name	Standard LPJS	
Manufacturer	Ainsworth Game Technology Limited	
Specification Number	44.YA005	
Category	PC (Progressive Controller)	
PC Type	STD (Standard Progressive Controller)	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standard Rev 1.2	
Controller Firmware Version	02.00.03.08	
Interface Card Firmware Version	1.44	
Jackpot Theme	Dollar King	
Operational Conditions
1.	The Paltronics Controller and Subsidiary Equipment Interface Card with specified firmware must operate as part of AGT’s Standard Linked Progressive Jackpot System with the ‘Dollar King’ game theme.
2.	The above-mentioned Jackpot Controller / SEI firmware must operate in conjunction with a ‘Dollar King’ game / shell combination.
3.	The system interface card must be enclosed in a sealed enclosure.	
Application Reference Number	44-A0628/S01	

Regression Tested Games with Previously Approved BIOS Software	
Game Details 1	
Game Name	Egypt Progressive	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Specification Number	06-BF000	
Category	GM (Gaming Machine)	
GM Type	iSAP (Integrated Stand-alone Progressive)	
Game Type	Spinning Reels	
Technical Standards 
Submission Standards	NS 9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard V4.18
NSW Jackpot Technical Standards Rev 1.1	
Platform/Cabinet Details	G-ENEX - Midway	
Game Details 2	
Game Name	Vampire And Beauty	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Specification Number	6.BF001	
Category	GM (Gaming Machine)	
GM Type	iSAP (Integrated Stand-alone Progressive)	
Game Type	Spinning Reels	
Technical Standards 
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18
NSW Jackpot Technical Standards Rev 1.1	
Platform/Cabinet Details	G-ENEX – G-Deluxe	
Game Details 3 	
Game Name	Bow Wow Bucks	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Specification Number	6.BF002	
Category	GM (Gaming Machine)	
GM Type	iSAP (Integrated Stand-alone Progressive)	
Game Type	Spinning Reels	
Technical Standards 
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18
NSW Jackpot Technical Standards Rev 1.1	
Platform/Cabinet Details	G-ENEX – G-Deluxe	

Continued
Game Details 4	
Game Name	Princess In Glass Slippers	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Specification Number	6.BF003	
Category	GM (Gaming Machine)	
GM Type	iSAP (Integrated Stand-alone Progressive)	
Game Type	Spinning Reels	
Technical Standards 
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18
NSW Jackpot Technical Standards Rev 1.1	
Platform/Cabinet Details	G-ENEX – G-Deluxe	
Game Details 5	
Game Name	Tokyo Rose	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Specification Number	6.F0013	
Category	GM (Gaming Machine)	
GM Type	Conventional	
Game Type	Spinning Reels	
Technical Standards 
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Platform/Cabinet Details	G-ENEX – Midway, Low Boy	
Game Details 6	
Game Name	Dragon’s Fortune	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Specification Number	6.F0014	
Category	GM (Gaming Machine)	
GM Type	Conventional	
Game Type	Spinning Reels	
Technical Standards 
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Platform/Cabinet Details	G-ENEX – Midway, Low Boy	

Continued
Game Details 7	
Game Name	Red Hot Chilli	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Specification Number	06-F0015	
Category	GM (Gaming Machine)	
GM Type	Conventional	
Game Type	Spinning Reels	
Technical Standards 
Submission Standards	NS 9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Platform/Cabinet Details	G-ENEX – Midway, Low Boy	
Game Details 8	
Game Name	Electra II	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Specification Number	06-F0016	
Category	GM (Gaming Machine)	
GM Type	Conventional	
Game Type	Spinning Reels	
Technical Standards 
Submission Standards	NS 9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Platform/Cabinet Details	G-ENEX – Midway, Low Boy	
Game Details 9	
Game Name	Shen Long	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Specification Number	6.F0017	
Category	GM (Gaming Machine) 	
GM Type	Conventional	
Game Type	Spinning Reels	
Technical Standards 
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Platform/Cabinet Details	G-ENEX – Midway, Low Boy	

Continued
Game Details 10	
Game Name	Scatter Pirates	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Specification Number	06-F0018	
Category	GM (Gaming Machine)	
GM Type	Conventional	
Game Type	Spinning Reels	
Technical Standards 
Submission Standards	NS 9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Platform/Cabinet Details	G-ENEX – Midway, Low Boy	
Game Details 11	
Game Name	Black Cat	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Specification Number	6.F0019	
Category	GM (Gaming Machine)	
GM Type	Conventional	
Game Type	Spinning Reels	
Technical Standards 
Submission Standards	NS 9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Platform/Cabinet Details	G-ENEX – Midway, Low Boy	
Game Details 12	
Game Name	Legend Of The Qin Dynasty	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Specification Number	6.F0020	
Category	GM (Gaming Machine)	
GM Type	Conventional	
Game Type	Spinning Reels	
Technical Standards 
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Platform/Cabinet Details	G-ENEX – Midway, Low Boy	

Continued
Game Details 13	
Game Name	Wild Hunters Tiger	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Specification Number	6.F0021	
Category	GM (Gaming Machine)	
GM Type	Conventional – Ante Bet	
Game Type	Spinning Reels	
Technical Standards 
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Platform/Cabinet Details	G-ENEX – Midway, Low Boy	
Game Details 14	
Game Name	The Last Emperor	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Specification Number	6.F0022	
Category	GM (Gaming Machine)	
GM Type	Conventional – Ante Bet	
Game Type	Spinning Reels	
Technical Standards 
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Platform/Cabinet Details	G-ENEX – Midway, Low Boy	
Game Details 15	
Game Name	Sabre Toothed Tiger	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Specification Number	6.F0023	
Category	GM (Gaming Machine)	
GM Type	Conventional – Ante Bet	
Game Type	Spinning Reels	
Technical Standards 
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Platform/Cabinet Details	G-ENEX – Midway, Low Boy	

Continued
Game Details 16	
Game Name	Big Challenge Mammoth	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Specification Number	6.F0024	
Category	GM (Gaming Machine)	
GM Type	Conventional – Ante Bet	
Game Type	Spinning Reels	
Technical Standards 
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Platform/Cabinet Details	G-ENEX – Midway, Low Boy	
Game Details 17	
Game Name	Giant Panda	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Specification Number	6.F0025	
Category	GM (Gaming Machine)	
GM Type	Conventional – Ante Bet	
Game Type	Spinning Reels	
Technical Standards 
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Platform/Cabinet Details	G-ENEX – Midway, Low Boy	
Game Details 18	
Game Name	Show Girl	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Specification Number	6.F0026	
Category	GM (Gaming Machine)	
GM Type	Conventional – Ante Bet	
Game Type	Spinning Reels	
Technical Standards 
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Platform/Cabinet Details	G-ENEX – Midway, Low Boy	

Continued
Game Details 19	
Game Name	Rock You Queen	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Specification Number	6.F0027	
Category	GM (Gaming Machine)	
GM Type	Conventional – Ante Bet	
Game Type	Spinning Reels	
Technical Standards 
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Platform/Cabinet Details	G-ENEX – Midway, Low Boy	
Game Details 20	
Game Name	San Guo Shi Dai (The Era of 3 Kingdoms)	
Manufacturer	Aruze Gaming Australia Pty Ltd	
Specification Number	6.F0028	
Category	GM (Gaming Machine)	
GM Type	Conventional – Ante Bet	
Game Type	Spinning Reels	
Technical Standards 
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Platform/Cabinet Details	G-ENEX – Midway, Low Boy	
Application Reference Number	06-A0307/S01	

New Monitoring System “KCMS”	
System Details 1	
System/Device Name	KCMS	
Manufacturer	Konami Australia Pty Ltd	
Specification Number	39-SET00	
Category	SE (Subsidiary Equipment)	
Technical Standards 
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
System Software Identifier	KCMS Release 3.19.2.28 – Patch 3.19.2.8
NAMB Version 2.11.7i	
System Details 2	
System/Device Name	KCMS – Remote Site	
Manufacturer	Konami Australia Pty Ltd	
Specification Number	39.SET01	
Category	SE (Subsidiary Equipment)	
Technical Standards 
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
System Software Identifier	KCMS Release 3.19.2.28 – Patch 3.19.2.8
NAMB Version 2.11.7i	
Specific Approval Conditions
1.	Konami must inform each purchaser and/or lessee of the KCMS system, in writing prior to or at the time of purchase/lease that the video streaming functionality be used responsibly or the video steaming function will be disabled.	
Operational Conditions
1.	The KCMS Wager Refund Functionality must be disabled during the installation stage.
2.	The Ticket expiry date in the system must be set to one (1) day during the installation stage.
3.	The KCMS must be configured in such a way that only authorised personnel have access to critical functions/parameters settings and sensitive information contained in the system.
4.	The KCMS must be provided and operated with a dedicated Uninterruptible Power Supply (UPS).  The UPS must provide sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption.
5.	The KCMS must be configured with automated backup facility.
6.	The KCMS interface card must be housed in a sealed enclosure, which requires access to the secure area of the Gaming Machine.
7.	Only those applications that are core to the KCMS operation, and evaluated by the GMTF and approved by the Authority are permitted to be configured.	
Additional Information
1.	The system is approved to operate in a dual port environment with any Paltronics Random Link Progressive Jackpot Systems that support jackpot CCCE transfer capability.	
Application Reference Number	39-A0908/S01	

Monitoring System “IGT Systems Club” Software Updates	
System/Device Name 1	IGT Systems Club	
Manufacturer	IGT (Australia) Pty Ltd	
Specification Number	18.SET02	
Category	SE (Subsidiary Equipment)	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
System Software Identifier	3.5	
Maximum number of connected gaming machines per Transaction Server 	300	
System/Device Name 2	IGT Systems Club – Remote Site	
Manufacturer	IGT (Australia) Pty Ltd	
Specification Number	18.SET04	
Category	SE (Subsidiary Equipment)	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
System Global Software Identifier	3.5	
The above-identified IGT Systems Club Version 3.5 is approved to operate with the following approved eCash Redemption Terminal:	
System/Device Name	eCash Redemption Terminal	
Specification Number	18.SER01	
Category	GSS (Gaming Support Systems)	
Submission Standards	NS 9.0 + NSW Appendix (dated 23/03/07)	
Technical Standards	NS 9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2
TITO Technical Standard V4.18	
Operational Conditions
1.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine.
2.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS).  The UPS must have sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption.  Desirably the system should be equipped with a “Smart” UPS capable of automatically shutting the system down in the case of a power failure.	
Application Reference Number	18-A1217/S01	

Monitoring System Software Update 	
Manufacturer	IGT (Australia) Pty Ltd	
System Name	IGT Systems Max	
Category 	Subsidiary Equipment	
Specification 	18.SET03	
Submission Standards	NS10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard V4.18	
System Software Identifier	3.2T	
The IGT Systems Max version 3.2T is approved to operate with the following Cash Redemption Terminal	
System Name	eCash Redemption Terminal	
Specification Number	18.SER01	
Category	Gaming Support Systems	
Submission Standards	NS 9.0 + NSW Appendix (dated 23/03/07)	
Technical Standards	NS 9.0 + NSW Appendix (dated 23/03/07)
NSW CPTS 2.2; TITO Technical Standard 4.18	
Controller Firmware	Version 02.00.03.08	
Interface Card Firmware	Version 1.21	
Specific Approval Conditions
1.	Use of the Xtra Credit facility is subject to the requirements of the Gaming Machine Act 2004 and Gambling and Racing Control (Code of Practice) Regulation 2002.
2.	The Xtra Credit functionality is limited to single venue use only.	
Operational Conditions
1.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine. 
2.	The “IGT Systems Max” is approved for use in a local area network (LAN) configuration only.
3.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS).  The UPS must have sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption.  Desirably the system should be equipped with a “Smart” UPS capable of automatically shutting the system down in the case of a power failure.
4.	The system must be configured in such a way that only authorised personnel have access to critical functions and sensitive information contained in the system.	
Application Reference Number	18.A1210/S01	

Jackpot Controller And Interface Card Software Bugfix	
System/Device Name	Standard LPJS –Mystical Temple	
Manufacturer	Konami Australia Pty Ltd	
Category	PC (Progressive Controller)	
PC Type	STD (Standard)	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standard  Rev 1.1	
Specification Number 	39.YA002	
Controller Firmware	Version 10	
Interface Card Firmware	Version 07	
Jackpot Theme	Mystical Temple	
List of previously approved games suitable for operation with the above-mentioned Standard LPJS and the Jackpot Display Controllers (optional):	
Game Name	Specification Number	Program ID	
Gold and Ruins Mystical Temple	39.H0043	GAR7NC10	
Relic Hunting Mystical Temple	39.H0044	REL7NB10	
Jungle Jewel Mystical Temple	39.H0045	JUN7NC10	
Incan Spirit Mystical Temple	39.H0046	INS7NA10	
Double Incan Riches Mystical Temple	39.H0047	DOI7NB10	
Specific Approval Conditions
1.	Konami must address the non compliance with Section 2.11.2.3 of the NSW jackpot Technical Standards rev 1.1 (Power switch not located in a secure enclosure of the controller) within 3 months of the date of this approval.  Konami must then retrofit any jackpot controllers sold within this period.	
Operational Conditions
1.	The system interface card must be enclosed in a sealed enclosure.	
Application Reference Number	39-A0919/S01	

Updated Standard Linked Progressive Jackpot System and Optional VGA Display Driver	
Device Name	Standard LPJS	
Manufacturer	Ainsworth Game Technology Limited	
Specification Number	44.YA005	
Category	PC (Progressive Controller)	
Category Type	STD (Standard Progressive Controller)	
Technical Standards 
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standard Rev 1.2	
Controller Firmware	Version 02.00.03.08	
Interface Card Firmware	Version 1.44	
Jackpot Theme	Rio Grande Rapids (Single Level)	
Operational Conditions
1.	The Paltronics Controller and Subsidiary Equipment Interface Card with specified firmware must operate as part of AGT’s Single Level Standard Linked Progressive Jackpot System with the ‘Rio Grande Rapids’ game theme.
2.	The above-mentioned Jackpot Controller / SEI firmware must operate in conjunction with an AGT’s Single Level ‘Rio Grande Rapids’ game / shell combination.
3.	The system interface card must be enclosed in a sealed enclosure.
4.	When using an overhead display with the VGA Display Driver, the following conditions must be complied:
a)	The system is to be run only under Windows XP operating system.
b)	The keyboard and mouse is to be attached only when performing maintenance and must be removed at all other times.
c)	The PC housing must have a provision to seal all points where the controller cables may be disconnected.
d)	The write filter application must be loaded on the hard drive at start up.	
Application Reference No.	44-A0648/S01; 44-A0643/S01	

New Standard Linked Progressive Jackpot System	
System/Device Name	Standard LPJS	
Manufacturer	Ainsworth Game Technology Limited	
Specification Number	44.YA006	
Category	PC (Progressive Controller)	
PC Type	STD (Standard Progressive Controller)	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standard Rev 1.2	
Controller Firmware	Version 02.00.03.08	
Interface Card Firmware	Version 1.44	
Jackpot Theme	Lights Camera Action	
Operational Conditions
1.	The Paltronics Controller and Subsidiary Equipment Interface Card with specified firmware must operate as part of AGT’s Single Level or Three Level “Standard LPJS” with the “Lights Camera Action” game theme.
2.	The above-mentioned Jackpot Controller / SEI firmware must operate in conjunction with a “Lights Camera Action” game / shell combination.
3.	The system interface card must be enclosed in a sealed enclosure.	
Application Reference Number	44-A0642/S01	

Monitoring System Software Update	
System Details 1:	
System name:	SYSTEM 7000	
Manufacturer:	Aristocrat Technologies Pty Ltd	
Category:	Subsidiary Equipment	
Specification Number	01-SET06	
System Details 2:	
System name:	SYSTEM 7000	
Manufacturer	Aristocrat Technologies Pty Ltd	
Category	Subsidiary Equipment	
Specification Number	01-SEZ07	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.20	
System Software Identifier	7.3.0.2	
The above-identified System 7000 is approved to operate with the following approved cash redemption terminals:	
Device Details 1	
Device name:	Sprintquip Cashback Centre	
Category	Subsidiary Equipment	
Specification Number	01-SER00	
Filename Version	TRMD_09_0K5.S19	
Device Details 2	
Device name;	eCash Cash Redemption Terminal 	
Category:	Subsidiary Equipment	
Specification number:	69-SER00	
Software Version:	V2.3.41.80	
Operational Conditions
1.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the Gaming Machine.	
Application Reference Number	01-A1251/S01, /S02	

ecash Redemption Terminal Software Update	
System Details:	
Device name:	ecash Cash Redemption Terminal	
Specification Number	69.SER00	
Manufacturer:	ecash Gaming Pty Ltd	
Category:	GSS (Gaming Support System)	
Category type:	Other (Gaming Machine Printed Ticket Redemption Station)	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.18	
The above-identified eCash Cash Redemption Terminal is approved to operate with the following monitoring system:	
System/Device Name:	System 7000	
Specification Number:	1.SET06	
System Software Version:	V7.3.0.2	
Operational Conditions
1.	The ecash Cash Redemption Terminal must operate with a host system at all times. 	
Application Reference Number	69-A0009/S01,	

System/Device Name	Multi Venue Jackpot System (NSW VWJS)	
Manufacturer	Paltronics Australia Pty Ltd	
Category	Subsidiary Equipment	
System Description	999 Jackpot Levels Multi Venue Linked Progressive Jackpot System with CCCE Jackpot Transfer and Dual Port functionality with up to 500 (100 unless communications systems have been tested) Inter-Venue Jackpot Linked Gaming Machines	
System Version	2.6.7.364	
Application Reference Number	ACT:SC/26-A0001 and 52-A0066/S01	
Technical Standards
	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standard Rev 1.2	
Submission Standards 	NS 10.0 + NSW Appendix (dated 14/01/09)	
System/Device Name	Multi Venue Jackpot System – Local Jackpot Controller	
Manufacturer	Paltronics Australia Pty Ltd	
Category	Subsidiary Equipment	
System Description	64 Jackpot Levels Mystery Linked Progressive Jackpot System with CCCE Jackpot Transfer and Dual Port functionality with up to 200 Attached Gaming Machines.	
System Version	2.00.04.01	
Application Reference Number	ACT:SC/26-A0001 and 52-A0066/S01	
Technical Standards
	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standard Rev 1.2	
Submission Standards 	NS 10.0 + NSW Appendix (dated 14/01/09)	
Operational Conditions
1)	The logic cage(s) housing the logic boards and other sensitive components of the MVJS (the MVJS Server and each attached local jackpot controller) must be closed and key-locked at all times, except during system maintenance or upgrade of the MVJS.
2)	The MVJS logic cages’ lock key(s) must be under the control of the venue manager.
3)	The MVJS must be configured to use a different session encryption key every 24 hours or more frequently. The session encryption key is the “password” used by the MVJS to encrypt all its communications between the MVJS Server, Local Jackpot Controllers and Config/Console Workstations.
4)	The ability to perform any server administration, system configuration, software modification and/or control the servers’ operation remotely must be disabled at all times, except during system maintenance or upgrade of the MVJS.
5)	Dedicated communication line (physical or logical) must be used for all communications between the MVJS Server, Local Jackpot Controllers and Config/Console Workstations.

6)	‘Rolled-up turnover’ is not approved for use in ACT and must be disabled at all times.	

Continued
7)	‘Offline play’ is not approved for use in ACT and must be disabled at all times. The parameters “Maximum Offline Play Time” and “Maximum Offline Turnover” must be set to zero for each operating jackpot level.
8)	The supplier must limit the number of inter-venue gaming machines operating with an MVJS to 100 unless the testing outlined in the OLGR Application Testing Report is carried out prior to increasing the number of inter-venue gaming machines. Please note that licencees cannot increase the number of gaming machines operated with an MVJS unless they have sought an amendment to their Multi User Permit.	

System/Device Name	Regressive Progressive Mystery Jackpot System 	
Manufacturer	Paltronics Australia Pty Ltd	
Category	Peripheral Equipment	
Category Type	Linked Jackpot System	
Specification	52-YC005	
Submission Standards 	NS 9.0 + NSW Appendix (dated 23/3/07)
NSW CPTS 2.2
NSW Jackpot Technical Standards Rev 1.1	
Technical Standards 	NS 9.0 + NSW Appendix (dated 23/3/07)
NSW CPTS 2.2
NSW Jackpot Technical Standards Rev 1.1	
Application Reference Number	52-A0044/S01	

Monitoring System ‘IGT Systems Club’ Software Update	
System/Device Name 1	IGT Systems Club	
Manufacturer	IGT (Australia) Pty Ltd	
Specification Number	18.SET02	
Category	SE (Subsidiary Equipment)	
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard V4.18	
System Software Identifier	3.4A	
Maximum number of connected gaming machines per Transaction Server 	300	
System/Device Name 2	IGT Systems Club – Remote Site	
Manufacturer	IGT (Australia) Pty Ltd	
 Specification Number	18.SET04	
Category	SE (Subsidiary Equipment)	
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard V4.18	
System Global Software Identifier	3.4A	
The above-identified IGT Systems Club Version 3.4A is approved to operate with the following approved cash redemption terminal:	
System/Device Name	eCash Cash Redemption Terminal	
Specification Number	69.SER00	
Category	GSS (Gaming Support Systems)	
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard V4.18	
CRT executable file Version	2.3.41.80 and above	
Operational Conditions
1.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine.
2.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS).  The UPS must have sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption.  Desirably the system should be equipped with a “Smart” UPS capable of automatically shutting the system down in the case of a power failure.	
Application Reference Number	18-A1212/S01	

Monitoring System ‘IGT Systems Club’ Software Update	
System/Device Name 1	IGT Systems Club	
Manufacturer	IGT (Australia) Pty Ltd	
Specification Number	18.SET02	
Category	SE (Subsidiary Equipment)	
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard V4.18	
System Software Identifier	3.5A	
Maximum number of connected gaming machines per Transaction Server 	300	
System/Device Name 2	IGT Systems Club – Remote Site	
Manufacturer	IGT (Australia) Pty Ltd	
 Specification Number	18.SET04	
Category	SE (Subsidiary Equipment)	
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard V4.18	
System Global Software Identifier	3.5A	
The above-identified IGT Systems Club Version 3.5A is approved to operate with the following approved eCash Redemption Terminal:	
System/Device Name	eCash Cash Redemption Terminal	
Specification Number	69.SER00	
Category	GSS (Gaming Support Systems)	
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard V4.18	
CRT executable file Version	2.3.41.80 and above	
Operational Conditions
1.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine.
2.	The system must be configured with automated backup facility.
3.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS).  The UPS must have sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption.  Desirably the system should be equipped with a “Smart” UPS capable of automatically shutting the system down in the case of a power failure.	
Application Reference Number	18-A1218/S01	

'Monitoring System ‘IGT Systems Club’ Software Update	
System/Device Name 1	IGT Systems Club	
Manufacturer	IGT (Australia) Pty Ltd	
Specification Number	18.SET02	
Category	SE (Subsidiary Equipment)	
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard V4.20	
System Software Identifier	3.6	
Maximum number of connected gaming machines per Transaction Server 	300	
System/Device Name 2	IGT Systems Club – Remote Site	
Manufacturer	IGT (Australia) Pty Ltd	
 Specification Number	18.SET04	
Category	SE (Subsidiary Equipment)	
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard V4.20	
System Global Software Identifier	3.6	
The above-identified IGT Systems Club Version 3.6 is approved to operate with the following approved cash redemption terminal:	
System/Device Name	eCash Cash Redemption Terminal	
Specification Number	69.SER00	
Category	GSS (Gaming Support Systems)	
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard V4.18	
CRT executable file Version	2.3.41.80 and above	
Operational Conditions
1.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine.
2.	The system must be configured with automated backup facility.
3.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS).  The UPS must have sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption.  Desirably the system should be equipped with a “Smart” UPS capable of automatically shutting the system down in the case of a power failure.	
Application Reference Number	18-A1222/S01	

Alternate Bill Acceptor	
System/Device Name	Bill Acceptor	
Manufacturer	Ainsworth Game Technology Limited	
Category	HW	
GM Type	Hardware Component	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2; TITO Technical Standard V4.20	
Bill Acceptor Details	AGT P/N: 025017 (CashCode FLS (with harness))
Harness    FL85.00.036-01	
Software Details	
Description	AGT P/N	Program ID	HMAC-SHA1	
Bill Acceptor	F025017-01	FLS-AU25-561730	ae4eed09 69bca740 20ee05c7
5b893dfb eacdffde	
Platform/Cabinet Details	A560-H – High Boy (with / without A560 Topper)
A560-L – Low Boy (with / without A560 Topper)
A560-L – Low boy (with 32” LCD Topper)	
Application Reference Number	44-A0613/S01	

Updated Standard Linked Progressive Jackpot System	
System/Device Name 1	Standard LPJS 	
Manufacturer	Ainsworth Game Technology Limited	
Specification Number	44.YA005	
Category	PC (Progressive Controller)	
PC Type	STD (Standard Progressive Controller)	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standard Rev 1.2	
LPJS Description	Standard Linked Progressive Jackpot Controller and Interface  Card with CCCE port sharing functionality	
Controller Firmware	Version 02.00.03.08	
Interface Card Firmware	Version 1.44	
Jackpot Theme	Player Paradise Platinum	
Operational Conditions
1.	The Paltronics Controller and Subsidiary Equipment Interface Card with specified firmware must operate as part of AGT’s Two Level “Standard LPJS” with the “Player Paradise Platinum” game theme.
2.	The above-mentioned Jackpot Controller / SEI firmware must operate in conjunction with a “Player Paradise Platinum” game / shell combination.
3.	The system interface card must be enclosed in a sealed enclosure.	
Application Reference Number	44-A0670/S01	

Generic Artwork Topper	
System/Device Name	Topper Artwork	
Manufacturer	Ainsworth Game Technology Limited 	
Category	GM (Gaming Machine)	
GM Type	Other (Artwork)	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)	
Artwork Details	
Topper Artwork	Content	
401279 Rev A	Hot New Game	
Platform/Cabinet Details	A560-H – High Boy
A560-L – Low Boy	
Previously approved games suitable for operation with the above-mentioned topper artwork:	All games that have been approved for operation on the A560-H and / A560-L platforms.	
Application Reference Number	44-A0695/S01	

Updated ATA Graphics Server Hyperlink & Mystery Link Configurations	
Device Name	Gen7 Vii Slant Platform Hyperlink & Mystery Link Configurations (incorporating the ATA Graphics Server)	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	GM (Gaming Machine)	
Category Type	Other (Dealer Display)	
Specification Number	01-SES00
01-SES01	
Submission Standards 
Technical Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2	
Platform/Cabinet Details	
c)	Hyperlink Configuration:	Gen7 Vii Slant – Casino Top (with in-machine LCD for Hyperlink) (Configured with Ticket Printer option)	
d)	Mystery Link Configuration:	Gen7 Vii Slant – Casino Top (with in-machine LCD for Hyperlink) (Configured with Ticket Printer option)	
Gen7 Vii Slant Platform Hyperlink & Mystery Link Configurations:	
a)	Hyperlink:	All Gen7 Vii Slant Casino Top cabinets + one Overhead Jackpot LCD / Plasma VGA Display)	
b)	Mystery Link:	All Gen7 Vii Slant Casino Top cabinets + one Overhead Jackpot LCD / Plasma VGA Display)	
List of previously approved games recommended for use on the Gen7 Vii Slant Platform Mystery Link Configurations:	
Game Name	Specification Number	Program ID	
Jackpot Catcher 	1.BF017	10261250	
Chariot Champion ($1) 	1.BF018	10261232	
Chariot Champion (50c)		10261349	
Polynesian Bounty – Emperor Penguin	1.BF019	10261082	
Harlequin Hearts – Emperor Penguin	1.BF020	10261101	
Lucky Strike – Silver & Gold Jackpots	1.BF022	10161392	
British Classic - World Turf Classics	1.BF023	10261348	
5 Dragons Legends (1c)	1.CF003	10161449	
5 Dragons Legends (2c)	1.CF004	10161450	
Queen of the Nile Legends (1c)	1.DF003	10361402	
Queen of the Nile Legends (2c)	1.DF004	10461514	
Stuck On You	1.F0068	10161187	
Dragon Emperor	1.F0070	10161174	
Don Quixote	1.F0071	10261193	
Jazee	1.F0073	10161172	
Bunny’s Rabbits	1.F0075	10261180	
More Hearts	1.F0076	10361268	
continued	

Game Name	Specification Number	Program ID	
More Chilli	1.F0077	10161387	
Love on the Nile	1.F0078	10261415	
Tiger Princess 	1.F0080	10261097	
Dollarsaur	1.F0081	10161338	
Pyramid Magic	1.F0082	10161502	
Tiger Garden	1.F0083	10261319	
Specific Approval Conditions
1.	The Acres Doli Protocol functionality is not a subject of this approval.
2.	The display content and access to display parameters must be implemented in a secure manner to prevent unauthorised access.  That is, access is limited to authorised Aristocrat personnel or authorised Aristocrat agents.
3.	The display is not to be used for the purpose of advertising or promotions.
4.	The jackpot pool values are to be displayed to the players generally most of the time (i.e. the display must keep players informed of the current state of the jackpot(s)).
5.	The number of Jackpot Levels displayed by the ATA Graphics Server of a selected Mystery Link should match the number of Jackpot Levels configured in the Jackpot Controller.
6.	The display is not to be used for feature or bonus games.
7.	The display material is not to be offensive and harm minimisation must be considered.	
Operational Conditions
1.	The ATA Graphics Server must be connected to an approved Linked Progressive Jackpot System as given above.
2.	The ATA Graphics Server active external I/O ports must be housed in a security cage fitted with a security seal to prevent connection or removal of data cables.	
Application Reference No.	01-A1279/S01	

Updated Hardware Assembly	
Device Name	Wing Lighting Board	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	GM (Gaming Machine)	
Category Type	Hardware Component	
Submission Standards 
Technical Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
	
Hardware Details	
Wing Lighting Board PCBA	ATA P/N: 494204 Issue D	
Platform/Cabinet Details	Gen7 Viridian Widescreen – Chop Top, Casino Top (with in machine LCD) (Configured with either Ticket printer and/or Hopper option)	
Application Reference No.	01-A1275/S01	

Monitoring System “IGT Systems Max” Software Update	
System Details 1	IGT Systems Max	
Manufacturer	IGT (Australia) Pty Ltd	
System Description	Data Gathering, Report Generating, Player Tracking / Bonus Points, Ticket In Ticket Out Validation, Dual Port Reconciliation, Xtra Credit, Pre-commitment and Group Ticket Functionality.	
Specification Number	18.SET03	
Category	SE (Subsidiary Equipment)	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.20	
System Software Identifier	3.3	
		
System Details 2	IGT Systems Max – Remote Site	
Manufacturer	IGT (Australia) Pty Ltd	
System Description	Data Gathering, Report Generating, Player Tracking / Bonus Points, Ticket In Ticket Out Validation, Dual Port Reconciliation, Xtra Credit, Pre-commitment and Group Ticket Functionality.	
Specification Number	18.SET05	
Category	GSS (Game Support Systems)	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.20	
System Software Identifier	3.3	
The above-identified IGT Systems Max is approved to operate with the following approved cash redemption terminal:	
System/Device Name	ecash Cash Redemption Terminal	
Device Description	Gaming Machine Printed Ticket Redemption Station	
Specification Number	69.SER00	
Category	GSS (Gaming Support Systems)	
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2, TITO,  Technical Standard 4.18	
CRT executable file Version:	2.3.41.80 and above	

continued	
Specific Approval Conditions:
1.	If Xtra Credit operation is enabled in a venue, the pre-commitment, the harm minimisation pop-up messages and the audible sound alert (Beep) are to be operational on all gaming machines connected to the system.
2.	Harm minimisation messages must include reference to the venue’s pre-commitment functionality and the availability of player activity statements.
3.	Gambling points must not be awarded to a member’s account as the result of promotions (gambling points are only accrued as the result of a player gambling on gaming machines).
4.	Only a venue’s authorised system administrator may adjust a member’s gambling account balance (a system message must inform the system administrator that gambling points are not to be awarded as the result of promotions).
5.	If multi-venue functionality is enabled, it is only approved to operate in amalgamated venues.	
Operational Conditions
1.	The system must be fitted with a compliance plate.
2.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the gaming machine.
3.	The system must be configured with automated backup facility.
4.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS).  The UPS must have sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption.  Desirably the system should be equipped with a “Smart” UPS capable of automatically shutting the system down in the case of a power failure.	
Application Reference Number	18-A1221/S01	

Updated Standard Linked Progressive Jackpot System and VGA Display Driver	
System/Device Name 	Standard LPJS 	
Manufacturer	Ainsworth Game Technology Limited	
Specification Number	44.YA005	
Category	PC (Progressive Controller)	
PC Type	STD (Standard Progressive Controller)	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standard Rev 1.2	
LPJS Description	Standard Linked Progressive Jackpot Controller and Interface Card with CCCE port sharing functionality	
Controller Firmware	Version 02.00.03.08	
Interface Card Firmware	Version 1.44	
Jackpot Theme	Dragon	
Device Details	
Device Name	Optional VGA Display Driver 	
Operational Conditions
1.	The Paltronics Controller and Subsidiary Equipment Interface Card with specified firmware must operate as part of AGT’s One Level “Standard LPJS” with the “Year of the Dragon” game theme.
2.	The above-mentioned Jackpot Controller / SEI firmware must operate in conjunction with a “Year of the Dragon” game / shell combination.
3.	The system interface card must be enclosed in a sealed enclosure.	
Application Reference Number	44-A0673/S01
44-A0702/S01	

Updated Standard Linked Progressive Jackpot System SEI Firmware	
System/Device Name 	Hyperlink LPJS (Max 504 EGM)	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Specification Number	01.YA002 (SLPJS)
01.SES00 (ATA Graphics Server)
1.SES01 (Thin Client ATA Graphics Server)	
Category	PC (Progressive Controller)	
PC Type	STD (Standard Progressive Controller)	
Technical Standards
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
NSW Jackpot Technical Standard Rev 1.2	
LPJS Description	Standard Linked Progressive Jackpot Controller and Interface Card with CCCE port sharing functionality	
Controller Firmware	Version 6.00	
Interface Card Firmware	Version 11.0 or 11.1	
Jackpot Themes	JAWS link
Bonus Link
FA FA FA Link
Bank Buster Link
Cash Express / Money Train Link
Beat the Bandits Link	
Specific Approval Conditions
This Hyperlink LPJS (Max 504 EGM) is approved to operate with hyperlink games that have been approved / authorised with the following Hyperlink ‘Link Progressive System’ Specification Numbers:	
Link Configurations	Gaming Machine Configurations	
Hyperlink LPJS Specification Numbers	Setting Ids	Jackpot Themes	BCV	Trigger Constants	
01-YH030	H0030001-H0030008	Cash Express / Money Train	1c	$275	
01-YH290	H0290001-H0290008			$350	
01-YH300	H0300001-H0300008			$425	
01-YH310	H0310001-H0310008			$500	
01-YH320	H0320001	Bank Buster	1c	$225.25	
01-YA001	H0030001-H0030008	Cash Express / Money Train	1c	$275	
	H0290001-H0290008			$350	
	H0300001-H0300008			$425	
	H0310001-H0310008			$500	
	H0320001	Bank Buster	1c	$225.25	
Operational Conditions
1.	.The ATA Graphics Server (1.SES00) or Thin Client ATA Graphics Server (1.SES01) must be connected to the above-mentioned Hyperlink Link Progressive Jackpot System.
2.	There must be at least one venue overhead display connected to the ATA Graphics Sever (1.SES00) or Thin Client ATA Graphics Server (1.SES01) so as to display pool values, the GMID / House Number of the winning gaming machine and the jackpot win amounts. 	
Application Reference Number	01-A1291/S01	

Gaming Machine Printed Ticket Redemption Station - Bugfix	
System/Device Name	Sprintquip Ultra Centre	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	SE (Subsidiary Equipment)	
Specification Number	1.SER01	
Submission Standards	NS 10.0 + NSW Appendix (dated 14/01/09)	
Technical Standards	NSW CPTS 2.2
TITO Technical Standard V4.18	
Software Details	
Description	Filename	Version	Type	CRC-32	
Sprintquip Ultra Centre Firmware	CRTManager.exe	1.0.0.365	Executable (HD)	FA877BA8	
Hardware Details: Platform Details	
Device	Description	Part Number	
PC (minimum requirement)		
Processor	Intel Celeron M 440 1.86GHz/FSB 
533/1M L2 Cache		
Memory	I Gb RAM (minimum)		
Hard Disk	40Gb		
Network	2x Intel 82573V Gigabit Ethernet		
-	Operating System	Microsoft Windows XP Embedded		
Cabinet	Sprintquip Ultra Centre	UC-1	
Note Dispenser	Talaris	NMD050	
Hoppers	Himecs	GH3200-A2	
Power Supplies	Power Distribution to all components	NMD – PS126 
Main – SETEC model no ATXG-450-2	
19” Open Frame Effinet	19” Touch Screen	IR touch screen USB model number E19U	
LCD Display	19” open frame gaming Effinet LCD screen	Effinet EFL 1902x	
PC	Fanless Industrial	Abbor F7000/CM1860 R1.0 part no BOX-PC-4-XSERIAL-V1.1	
Thermal Ticket/Note Reader	Cashcode Validator	FL-0439AU1519, with FLC103 stacker using AU1519 firmware	
Thermal Printer	Future Logic	PSA-66-ST2RU	
Logic PCB	RS232 Interface	SQUCV1.00	

Continued
The following are approved monitoring systems that are approved to operate with the above-identified Sprintquip Ultra Centre:	
System Details 1:		
System Name	System 6000	
Category	SE (Subsidiary Equipment)	
Specification Number	1.SEBT0 & 1.SET05	
System Software Version Identifier	6.3.12 and above	
System Details 2	
System Name	System 7000	
Category	SE (Subsidiary Equipment)	
Specification Number	1.SET06	
System Software Version Identifier	7.2.100.26 and above	
System Details 3	
System Name	Dacom 5000E	
Category	SE (Subsidiary Equipment)	
Specification Number	1.SETX1	
System Software Version Identifier	Dacom 4.40 and above	
Operational Conditions
1.	The Sprintquip Ultra Centre’s screen must be configured to display the Problem Gambling Notice message.	
Application Reference Number	01-A1296/S01	

Monitoring System Software Update 	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
System Name 1	System 7000	
System Description	Data Gathering, Report Generating, Player Tracking / Bonus Points and Ticket In Ticket Out Validation, Dual Port Reconciliation and Take a Break	
Category	Subsidiary Equipment	
Specification Number	1.SET06	
System Name 2	System 7000	
System Description	Data Gathering, Report Generating and Player Loyalty / Bonus Points	
Category	Subsidiary Equipment	
Specification Number	1.SEZ07	
Submission Standards
Technical Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.20	
System software Identifier	7.3.0.3	
The above-identified System 7000 is approved to operate with the following approved cash redemption terminals	
Device Name 1	Sprintquip Cashback Centre	
Category	Subsidiary Equipment	
Specification Number	1.SER00	
Device Name 2	Sprintquip Ultra Centre	
Category	Subsidiary Equipment	
Specification Number	1.SER01	
Device Name 3	eCash Cash Redemption Terminal	
Category	Subsidiary Equipment	
Specification Number	69-SER00	
Operational Conditions
1.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the Gaming machine.	
Application Reference Number	01-A1289/S01 /S02	

Monitoring System Software Update 	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
System Name 1	System 7000	
System Description	Data Gathering, Report Generating, Player Tracking / Bonus Points and Ticket In Ticket Out Validation, Dual Port Reconciliation and Take a Break	
Category	Subsidiary Equipment	
Specification Number	1.SET06	
System Name 2	System 7000	
System Description	Data Gathering, Report Generating and Player Loyalty / Bonus Points	
Category	Subsidiary Equipment	
Specification Number	1.SEZ07	
Submission Standards
Technical Standards	NS 10.0 + NSW Appendix (dated 14/01/09)
NSW CPTS 2.2
TITO Technical Standard V4.20	
System software Identifier	7.3.0.4	
The above-identified System 7000 is approved to operate with the following approved cash redemption terminals	
Device Name 1	Sprintquip Cashback Centre	
Category	Subsidiary Equipment	
Specification Number	1.SER00	
Device Name 2	Sprintquip Ultra Centre	
Category	Subsidiary Equipment	
Specification Number	1.SER01	
Device Name 3	eCash Cash Redemption Terminal	
Category	Subsidiary Equipment	
Specification Number	69-SER00	
Operational Conditions
1.	The system interface card must be housed in a sealed enclosure, which requires access to the secure area of the Gaming machine.	
Application Reference Number	01-A1309/S01