Australian Capital Territory
Gaming Machine (Peripheral Equipment) Approval 2015 (No 1)
Notifiable instrument NI2015– 49
made under the  
Gaming Machine Act 2004, section 69 (Approval of gaming machines and peripheral equipment)

1	Name of instrument
This instrument is the Gaming Machine (Peripheral Equipment) Approval 2015 (No 1).

2	Commencement 
This instrument commences the day after the date of notification.

3	Approval
I approve the peripheral equipment described in the attached Schedule to this instrument.  

Maureen Ogilvie
Delegate
ACT Gambling and Racing Commission

3 February 2015

New Standard Linked Progressive Jackpot System	
System Name 	Standard LPJS – Duo Fu Wa Super 88	
Manufacturer	Bally Technologies ANZ Pty Ltd	
Specification Number	35.YA003	
Category	PC (Progressive Controller)	
PC Type	Standard Progressive Controller	
Technical Standards
Submission Standards	NS 10.3 + NSW Appendix (dated 24/04/2013)
NSW CPTS 2.3
NSW Jackpot Technical Standard Rev 1.3
TITO Technical Standard V4.20	
LPJS Description	Standard Linked Progressive Jackpot Controller and Interface Card with CCCE port sharing functionality	
Controller Firmware	Version 02.00.03.09 or 02.01.00.24	
Interface Card Firmware	Version 1.27 or 2.17	
Jackpot Theme	More Lucky Dolls	
Software Details – 1	
Jackpot Controller	OLJ-02-00-03-09O	
	OLJ-02-00-03-09E	
Parameter EPROM	DFW Super88 JP Parameters v2.bin	
Parameter EPROM with no header	DFW Super88 JP Parameters v2-noheader.bin	
Software Details - 2	
Jackpot Controller	OLJ-02.01.00.24-o	
	OLJ-02.01.00.24-E	
	OLJ-02.01.00.24 (binary)	
Parameter EPROM	DFW Super88 JP Parameters v2.bin	
Parameter EPROM with no header	DFW Super88 JP Parameters v2-noheader.bin	
Specific Approval Conditions
1.	The Paltronics Controller and Subsidiary Equipment Interface Card with specified firmware must operate as part of Bally Technologies ANZ’s “Duo Fu Wa Super 88” Standard LPJS with the same game theme.
2.	The above-mentioned Jackpot Controller / SEI firmware must operate in conjunction with a “Duo Fu Wa Super 88” game / shell combination.
3.	The system interface card must be enclosed in a sealed enclosure.	
Application Reference Number	35-A0951/S01
35-A0970/S01