Australian Capital Territory
Gaming Machine (Peripheral Equipment) Approval 2015 (No 5)
Notifiable instrument NI2015–499
made under the  
Gaming Machine Act 2004, section 69 (Approval of gaming machines and peripheral equipment)

1	Name of instrument
This instrument is the Gaming Machine (Peripheral Equipment) Approval 2015 (No 5).

2	Commencement 
This instrument commences the day after the date of notification.

3	Approval
I approve the peripheral equipment described in the attached Schedule to this instrument.  

Lesley Maloney
Delegate
ACT Gambling and Racing Commission

24 August 2015

Updated Standard  / Hyperlink LPJS Controller Software	
System/Device Name 	Standard / Hyperlink LPJS (Max 504 EGM)	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Specification Number	1.YA002 (SLPJS)
1.SES00 (ATA Graphics Server)
1.SES01 (Thin Client Graphics Server)
1.SES03 (Kontron ATA Graphics Server)	
Category	PC (Progressive Controller)	
Technical Standards
Submission Standards	NS 10.3 + NSW Appendix (dated 24/04/13)
NSW CPTS 2.4; NSW Jackpot Technical Standard Rev 1.3	
LPJS Description	Standard Linked Progressive Jackpot Controller and Interface Card with CCCE port sharing functionality	
Controller Firmware	Version 6.07	
Interface Card Firmware	Version 11.1	
Jackpot Themes	JAWS link (Hyperlink)
Bonus Link (Hyperlink)
FA FA FA Link (Hyperlink) 
Bank Buster Link (Hyperlink)
Cash Express / Money Train Link (Hyperlink)
Beat the Bandits Link (Hyperlink)
Keys of Fortune Link (Standard)
Cash Express Link (2c) (Hyperlink)
Ca$h Explo$ion Link (Standard)
Lightning Link (1c) (Standard)	
Specific Approval Conditions
1.	This Standard/Hyperlink LPJS (Max 504 EGM) is approved to operate with hyperlink games that have been approved / authorised with the following Hyperlink ‘Link Progressive System’ Specification Numbers:	
Link Configurations	Gaming Machine Configurations	
Hyperlink LPJS Specification Numbers	Setting Ids	Jackpot Themes	BCV	Trigger Constants	
01-YH030	H0030001-H0030008	Cash Express / Money Train	1c	$275	
01-YH290	H0290001-H0290008			$350	
01-YH300	H0300001-H0300008			$425	
01-YH310	H0310001-H0310008			$500	
01-YH320	H0320001	Bank Buster	1c	$225.25	
01-YA001	H0030001-H0030008	Cash Express / Money Train	1c	$275	
	H0290001-H0290008			$350	
	H0300001-H0300008			$425	
	H0310001-H0310008			$500	
	H0320001	Bank Buster	1c	$225.25	
2.	The ATA Graphics Server (1.SES00) or Thin Client ATA Graphics Server (1.SES01) must be connected to the above-mentioned Standard / Hyperlink Link Progressive Jackpot System.
3.	There must be at least one venue overhead display connected to the ATA Graphics Sever (1.SES00) or Thin Client ATA Graphics Server (1.SES01) so as to display pool values, the GMID / House Number of the winning gaming machine and the jackpot win amounts.	
Application Reference Number	01-A1526/S01	

Updated ATA Graphics Server Software	
System Name 	Kontron ATA Graphics Server / Thin Client ATA Graphics Server	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	Gaming Machine	
Type	Graphics Server	
Specification Number	1.SES03 
1.SES01	
Technical Standards
Submission Standards	NS 10.3 + NSW Appendix (dated 24/04/13)
NSW CPTS Rev 2.4;
NSW Jackpot Technical Standard Rev 1.3	
Additional Graphics Themes	
Part Number	575392-146 (Lightning Link)	
Link details	Standard Link 1 level Jackpot	
ATA Graphics Server Details	
Thin Client ATA Graphics Server (1.SES01)	P/N: ATA 442027_4	
Kontron ATA Graphics Server (1.SES03)	P/N: ATA 442300	
Specific Approval Conditions
1.	The Acres Doli Protocol functionality is not a subject of this approval.
2.	The number of Jackpot Levels displayed by the ATA Graphics Server of a selected Mystery Link should match the number of Jackpot Levels configured in the Jackpot Controller.
3.	Each Thin Client ATA Graphics Server (P/N: ATA 442027_4) operating within a venue must be authorised with the Specification Number: 1.SES01.
4.	Each Kontron ATA Graphics Server (P/N: ATA 442300) operating within a venue must be authorised with the Specification Number: 1.SES03.
5.	The Thin Client ATA Graphics Server / Kontron ATA Graphics Server must be connected to an approved Standard / Hyperlink / Random Link Progressive Jackpot System as given above. 
6.	The Thin Client ATA Graphics Server / Kontron ATA Graphics Server active external I/O ports must be housed in a security cage fitted with a security seal to prevent connection or removal of data cables.	
Application Reference Number	01-A1527/S01	

In-Venue Gaming System Software Update ‘IGT Systems Club’	
System Name 1	IGT Systems Club 	
Manufacturer	IGT (Australia) Pty Ltd	
System Description	Data Gathering, Report Generating, Player Tracking / Bonus Points, Ticket In Ticket Out Validation, Group Ticket, Xtra Credit, Pre-commitment and Harm Minimisation Messages and iBreak functionality.	
Specification Number	18.SET02	
Category	In-Venue Gaming System (Subsidiary Equipment)	
Submission Standards	NS 10.3 + NSW Appendix (dated 24/11/11)	
Technical Standards	NSW CPTS 2.3; TITO TS V4.20	
System Software ID	4.0	
System Name 2	IGT Systems Club – Remote Site	
System Description	Data Gathering, Report Generating, Player Tracking / Bonus Points, Ticket In Ticket Out Validation, Group Ticket, Xtra Credit, Pre-commitment and Harm Minimisation Messages and iBreak functionality.	
Specification Number	18.SET04	
Category	In-Venue Gaming System (Subsidiary Equipment)	
Submission Standards	NS 10.3 + NSW Appendix (dated 24/11/11)	
Technical Standards	NSW CPTS 2.3; TITO TS V4.20	
System Software ID	4.0	
Specific Approval Conditions
1.	The Kiosk promotion feature must be disabled. The ‘Maximum promotional Bonus’ value must be set at zero(0).
2.	Use of the Xtra Credit facility is subject to the requirements of the Gaming Machine Act 2004 and the Gambling and Racing Control (Code of Practice) Regulation 2002. 
3.	If multi-venue functionality is enabled, it is only approved to operate in amalgamated venues.
4.	The system must be configured with automated backup facility.
5.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS). The UPS must have sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption. Desirably the system should be equipped with a “Smart” UPS capable of automatically shutting the system down in the case of a power failure.	
Application Reference Number	18-A1273/S01, 18-A1273/S02