Australian Capital Territory
Gaming Machine (Peripheral Equipment) Approval 2015 (No 9)
Notifiable instrument NI2015–644
made under the  
Gaming Machine Act 2004, section 69 (Approval of gaming machines and peripheral equipment)

1	Name of instrument
This instrument is the Gaming Machine (Peripheral Equipment) Approval 2015 (No 9).

2	Commencement 
This instrument commences the day after the date of notification.

3	Approval
I approve the peripheral equipment described in the attached Schedule to this instrument.  

Maureen Ogilvie
Delegate
ACT Gambling and Racing Commission

13 November 2015

Updated A560 LPJS Controller Base Firmware	
System Name 	A560 Link Progressive Jackpot System	
Manufacturer	Ainsworth Game Technology Limited	
Category	Progressive Controller	
Specification Number	44.YC000 – Random (Mystery) LPJS
44.YA007 – Standard LPJS	
Technical Standards
Submission Standards	NS 10.3 + NSW Appendix (dated 24/04/13); NSW CPTS 2.4
 ILGA Circular (dated 03/07/15)
NSW Jackpot Technical Standard Rev 1.3	
LPJS Description	Random and Standard Linked Progressive Jackpot System with CCCE Jackpot Transfer and Port Sharing Functionality.	
Software Details 	
Description	Firmware	
LPJS Controller	
Link Controller Base	X522082J	
Link Controller Game	NXC0332C	
Link Controller BIOS	A004E002	
Display Controller 1	
Display Controller Base	DCO3202D	
Display Media Files	N/A	
Display Controller 2	
Display Controller Base	DMO1202F	
Display Media Files	N/A	
Specific Approval Conditions
1.	The A560 Link Progressive Jackpot System and Subsidiary Equipment Interface card with the specified firmware must operate in conjunction with Ainsworth games.
2.	The A560 Link Progressive Jackpot System is approved to configure up to 8 progressive jackpot groups only.
3.	Ainsworth must ensure that for each Progressive Jackpot Group enrolled on to the A560 Link Progressive Jackpot System, a new serial number is assigned.
4.	If ‘Double Shot Favourites’ Standard LPJS is configured, the Display Controller with Media firmware version ‘NXD0181B’ or later must be enabled.	
Application Reference Number	44-A0975/S01	

Alternate Video Card for the Kontron ATA Graphics Server	
System Name 	Kontron ATA Graphics Server	
Manufacturer	Aristocrat Technologies Australia Pty Ltd	
Category	Gaming Machine	
Category Type	Graphics Server	
Technical Standards
Submission Standards	NS 10.3 + NSW Appendix (dated 24/04/13); NSW CPTS Rev 2.4; NSW Jackpot Technical Standards Rev 1.3 	
Hardware Details 	
Description	Part Number	
Kontron ATA Graphics Server (Link Kit):
•	Kontron ID
o	Processor
o	Chipset
o	Memory
o	Disk Memory
o	Graphics Adapter

o	BIOS	ATA 442300
KIB-LP-340-HM65-A
Intel Celeron B810 1600MHz
Intel HM65 Platform Controller Hub
DDR3 SODIMM 2GB
SSD 16GB
a)	Radeon HD6570 1GB DVI HDMI
b)	Radeon HD7570 1GB DVI / HDMI
AMI	
LPJS Details	
LPJS Type	Software Version	Specification number	
Random with Mk6 & Gen7 platforms	
a)	Mikohn LPJS	CCCE44	32.YC000	
b)	Paltronics LPJS	52XO199C / 52XE199C
XST0207O / XST0207E	52.YC000	
c)	Paltronics LPJS	XSE0116O / XSE0116E	52.YC001	
Standard with Mk7 & Gen8 platforms	
Standard LPJS	SHL0404O / SHL0404E	1.YA001	
	SHL0603O / SHL0603E	1.YA002	
	SHL0604O / SHL0604E	1.YA002	
	SHL0605O / SHL0605E	1.YA002	
	SHL0607O / SHL0607E	1.YA002	

Cont.....
Hyperlink with Mk6 & Gen7 platforms	
a)	Hyperlink	SHL03280 / SHL0328E	1.YA000
1.YH030
1.YH050
1.YH060 to 1.YH170	
	a)	SHL0330O / SHL0330E
b)	SHL0332O / SHL0332E	1.YA000
1.YH030
1.YH050
1.YH060 to 1.YH170
1.YH280
1.YH290 to1.YH310	
	SHL0335O / SHL0335E	1.YA000
1.YH030
1.YH050
1.YH060 to 1.YH170
1.YH280
1.YH290 to1.YH310
1.YH320
1.YHD00	
	SHL0404O / SHL0404E	1.YA001	
	SHL05010 / SHL0501E	1.YA002	
	SHL0502O / SHL0502E	1.YA002	
	SHL0505O / SHL0505E	1.YA002	
	SHL0600O / SHL0600E	1.YA002	
	SHL0603O / SHL0603E	1.YA002	
	SHL0604O / SHL0604E	1.YA002	
	SHL0605O / SHL0605E	1.YA002	
	SHL0607O / SHL6507E	1.YA002	
Specific Approval Conditions
1.	Each Kontron ATA Graphics Server operating within a venue must be authorized with the corresponding Specification Number.
2.	The Kontron ATA Graphics Server must be connected to an approved Standard / Hyperlink / Random Linked Progressive Jackpot System as given above.
3.	The Kontron ATA Graphics Server active external I/O ports must be housed in a security cage fitted with a security seal to prevent connection or removal of data cables.
4.	The Acres Doli Protocol functionality is not a subject of this approval.
5.	The display content and access to display parameters must be implemented in a secure manner to prevent unauthorized access. That is, access is limited to authorized Aristocrat personnel or authorized Aristocrat agents.
6.	The jackpot pool values are to be displayed to the players generally most of the time (i.e. the display must keep players informed of the current state of the jackpots).
7.	The number of jackpot levels displayed by the Kontron ATA Graphics Server of a selected Mystery Link should match the number of jackpot levels configured in the jackpot controller.
8.	The display is not to be use for feature or bonus games.
9.	The display is not to be offensive and harm minimization must be considered. 	
Application Reference Number	01-A1589/S01