Australian Capital Territory
Gaming Machine Approval 2016 (No 21)
Notifiable instrument NI2016–384
made under the 
Gaming Machine Act 2004, section 69 (Approval of gaming machines and peripheral equipment)

1	Name of instrument
This instrument is the Gaming Machine Approval 2016 (No 21).

2	Commencement 
This instrument commences the day after the date of notification.

3	Approval
I approve the gaming machine(s) described in the attached Schedule to this instrument.

Lesley Maloney
Delegate
ACT Gambling and Racing Commission

22 July 2016 

For further information please contact the approved supplier.

IGT (Australia) Pty Ltd	
Subject: New Gaming Machine	
Game Name	Temple of the Sun	
Specification Number	18.BG003	
Application Reference No.	18-A5507/S01	
Specific Approval Conditions
After a RAM Clear, in the machine configuration menu, the MDB Type must be V0106 to enable functions supported in the CPTS 2.4.	

IGT (Australia) Pty Ltd	
Subject: New Gaming Machine	
Game Name	Temple of the Sun	
Specification Number	18.BG007	
Application Reference No.	18-A5509/S01	
Specific Approval Conditions
After a RAM Clear, in the machine configuration menu, the MDB Type must be V0106 to enable functions supported in the CPTS 2.4.	

IGT (Australia) Pty Ltd	
Subject: New Gaming Machine	
Game Name	Temple of the Moon	
Specification Number	18.BG001	
Application Reference No.	18-A5508/S01	
Specific Approval Conditions
After a RAM Clear, in the machine configuration menu, the MDB Type must be V0106 to enable functions supported in the CPTS 2.4.	

IGT (Australia) Pty Ltd	
Subject: New Gaming Machine	
Game Name	Temple of the Moon	
Specification Number	18.BG006	
Application Reference No.	18-A5510/S01	
Specific Approval Conditions
After a RAM Clear, in the machine configuration menu, the MDB Type must be V0106 to enable functions supported in the CPTS 2.4.	

IGT (Australia) Pty Ltd	
Subject: New Gaming Machine	
Game Name	Tomb of the King	
Specification Number	18.DG016	
Application Reference No.	18-A5465/S01	
Specific Approval Conditions
After a RAM Clear, in the machine configuration menu, the MDB Type must be V0106 to enable functions supported in the CPTS 2.4.	
IGT (Australia) Pty Ltd	
Subject: New Gaming Machine	
Game Name	Multistar Champion Series Black	
Specification Number	18.BG015	
Application Reference No.	18-A5466/S01	
Specific Approval Conditions
•	The Dynamic Button Panel Assembly must be installed for the abovementioned game when operating on the given platform.
•	During EGM configuration the option Data Block Extn and MDB Type 1.06 must be selected to support the additional classes defined in CPTS 2.4.
•	The above game may operate with the optional Multilayer Display on the AVP BC20 Video Top platform.	

IGT (Australia) Pty Ltd	
Subject: Supporting Software (Platform, OS, BIOS)	
Game Name	Crystal Core Platform	
Specification Number	Software Details 
PLATFORM_00000163.vhd; PLATFORM_00000163. vhd.sig	
Application Reference No.	518-A5511/S01	
Specific Approval Conditions
Nil.	

IGT (Australia) Pty Ltd	
Subject: Gaming Machine	
Game Name	UG20 Conversion Kit	
Specification Number	N/A	
Application Reference No.	18-A1283/S01	
Specific Approval Conditions
Nil.	

eBet Gaming Systems	
Subject: New Multi Game Gaming Machine Game	
Game Name	Game Chest 2	
Specification Number	50.C0001	
Application Reference No.	50-A0217/S01	
Specific Approval Conditions
Nil.	

eBet Gaming Systems	
Subject: New Gaming Machine	
Game Name	Kiss	
Specification Number	50.F0083	
Application Reference No.	50-A0218/S01	
Specific Approval Conditions
Nil.	

Ainsworth Game Technology	
Subject: New Gaming Machine	
Game Name	Robinson Crusoe	
Specification Number	44.HQG10	
Application Reference No.	44-A1048/S01	
Specific Approval Conditions
•	The abovementioned game must be authorised at a BVC of 1 cent only.
•	The abovementioned Standard Linked Progressive Game must operate in conjunction with the Standard Linked Progressive Jackpot System, Spec No. 44.YA007, with the approved Cash Adventures jackpot settings as included in the Link Controller Game Firmware NXC0332G and operating with the Link Controller Base Firmware X522082J and Link Controller BIOS A004E002.
•	The abovementioned game must be operated with the 15 Button OLED Panel on the A560X-ST platform.
•	The abovementioned game must be operated with the 15 Button OLED panel or 15 inch LCD on the A600-H platform.
•	The abovementioned game can be operated with the optional 24” or 27” LCD Topper on the A560X-ST platforms.
•	The abovementioned game can be operated with the optional 21.5” or 24” or 27” LCD Topper on the A600-H platforms.