Australian Capital Territory
Gaming Machine (Peripheral Equipment) Approval 2014 (No 15)
Notifiable instrument NI2014–605
made under the  
Gaming Machine Act 2004, section 69 (Approval of gaming machines and peripheral equipment)

1	Name of instrument
This instrument is the Gaming Machine (Peripheral Equipment) Approval 2014 (No 15).

2	Commencement 
This instrument commences the day after the date of notification.

3	Approval
I approve the peripheral equipment described in the attached Schedule to this instrument.  

Maureen Ogilvie
Delegate
ACT Gambling and Racing Commission

26 November 2014

Regression Tested Jackpot ‘Rio Grande Rapids – Single Level LPJS’	
System Name 	Standard LPJS	
Manufacturer	Ainsworth Game Technology Limited	
Category	Progressive Controller	
Type	Standard Progressive Controller	
Technical Standards
Submission Standards	NS 10.3 + NSW Appendix (dated 24/04/13);
NSW JP TS Rev 1.3; NSW CPTS 2.3	
LPJS Description	Standard Linked Progressive Jackpot Controller with CCCE Port Sharing Functionality	
Controller Firmware	Version 02. 01.00 24	
Interface Card Firmware (PALA5)	Version 2.21	
Jackpot Themes Details:	
Jackpot Themes	Standard LPJS Specification Number	
Classic	44.YA005	
Rio Grande Rapids	44.YA005	
Rio Grande Rapids	44.YA005 (single level)	
Player Paradise	44.YA005	
Player Paradise Platinum	44.YA005	
Dollar King	44.YA005	
Dragon	44.YA005	
Lights Camera Action	44.YA006	
Jackpot Zone	44.YA008	
Fortune Ox	44.YA008	
Application Reference Number	44-A0884/S01	

In-Venue Gaming System Functionalities Update ‘Player Account and Transfer Card’ 	
Manufacturer	eBet Gaming Systems Pty Ltd	
System Name 1	eBet Netcash CCCE SQL	
System Description	Data Gathering, Report Generation, Promotional, Player Account, TITO, Alternate TITO, Dual Port Reconciliation, Breakaway and Transfer Card functionalities. 	
Specification Number	50.CABT0	
System Name 2	eBet Netcash CCCE SQL	
System Description	Data Gathering, Report Generation, Promotional, Player Account, TITO, Alternate TITO, Dual Port Reconciliation and Transfer Card functionalities.	
Specification Number	50.CAPT0	
System Name 3	eBet Netcash CCCE SQL	
System Description	Data Gathering, Report Generation, Promotional, TITO, Alternate TITO and Transfer Card functionalities.	
Specification Number	50.SET02	
System Name 4	eBet Netcash CCCE SQL	
System Description	Data Gathering, Report Generation and Promotional.	
Specification Number	50.SEZX5	
Category	Subsidiary Equipment	
Submission Standards
Technical Standards	NS 10.3 + NSW Appendix (dated 24/04/13)
NSW CPTS 2.3; TITO TS V4.20	
System Software Identifier	V2.0.39	
System Name 5	eBet Netcash CCCE SQL with GMI	
System Description	Data Gathering, Report Generation, Promotional, Player Account, Dual Port Reconciliation and Transfer Card functionalities.	
Specification Number	50.CAP02	
System Details 6	eBet Netcash CCCE SQL with Turbo 4000 Wedge	
System Description	Data Gathering, Report Generation, Promotional, Player Account, Dual Port Reconciliation and Transfer Card functionalities.	
Specification Number	50.CAP03	
The above-identified eBet Netcash CCCE SQL system is approved to operate with the following approved cash redemption terminals:	
System Details 1	Sprintquip Cashback Centre	
System Description	Gaming Machine Printed Ticket Redemption Station	
Specification Number	50.SER00	
Category	Subsidiary Equipment	
Software Version	TRMD4_03_0K5.S19 or later	

Continued
System Details 2	eCash Cash Redemption Terminal	
System Description	Gaming Machine Printed Ticket Redemption Station	
Specification Number	69-SER00	
Category	Subsidiary Equipment	
Software Version	V2.3.41.80 or later	
Specific Approval Conditions
The ‘Sprintquip Cashback Centre’ and the ‘eCash Cash Redemption Terminal’ are not subjects of this approval. 	
Operational Conditions
The only cashless gaming system approved for use in the ACT is a Ticket-In Ticket Out system.	
Application Reference Number	50-A0212/S01, 50-A0212/S02	

In-Venue Gaming System Software Update ‘IGT Systems Club’	
System Name 1	IGT Systems Club 	
System Description	Data Gathering, Report Generating, Player Tracking / Bonus Points, Ticket In Ticket Out Validation, Group Ticket, Xtra Credit, Pre-commitment and Harm Minimisation Messages and iBreak functionality.	
Specification Number	18.SET02	
Category	In-Venue Gaming System (Subsidiary Equipment)	
Submission Standards	NS 10.3 + NSW Appendix (dated 24/11/11)	
Technical Standards	NSW CPTS 2.3; TITO TS V4.20	
System Global ID	3.9	
System Name 2	IGT Systems Club – Remote Site	
System Description	Data Gathering, Report Generating, Player Tracking / Bonus Points, Ticket In Ticket Out Validation, Group Ticket, Xtra Credit, Pre-commitment and Harm Minimisation Messages and iBreak functionality.	
Specification Number	18.SET04	
Category	In-Venue Gaming System (Subsidiary Equipment)	
Submission Standards	NS 10.3 + NSW Appendix (dated 24/11/11)	
Technical Standards	NSW CPTS 2.3; TITO TS V4.20	
System Global ID	3.9	
Specific Approval Conditions
1.	Use of the Xtra Credit facility is subject to the requirements of the Gaming Machine Act 2004 and the Gambling and Racing Control (Code of Practice) Regulation 2002. 
1.	If multi-venue functionality is enabled, it is only approved to operate in amalgamated venues.
2.	The system must be configured with automated backup facility.
3.	The system must be provided and operated with a dedicated uninterrupted power supply (UPS). The UPS must have sufficient capacity to allow the system, and any associated critical elements, to be shut down gracefully in the event of a power interruption. Desirably the system should be equipped with a “Smart” UPS capable of automatically shutting the system down in the case of a power failure.
4.	The only cashless gaming system approved for use in the ACT is a Ticket-In Ticket Out system.	
Application Reference Number	18-A1268/S01	

Random Link Progressive Jackpot System Software Update	
System Name 1	Multi-Venue Jackpot System – Server (NSW Venue Wide Jackpot System)	
Manufacturer	Paltronics Australasia Pty Ltd	
Category	Subsidiary Equipment	
Specification Number	52.YC002	
System Description	999 Jackpot Levels Multi Venue Linked Progressive Jackpot System with CCCE Jackpot Transfer and Dual Port functionality with up to 500 (100 unless communications systems have been tested) Inter-Venue Jackpot Linked Gaming Machines	
Technical Standards
Submission Standards	NS 10.3 + NSW Appendix (dated 24/04/13)
NSW CPTS 2.3; NSW JP TS Rev 1.3	
System Version	2.9 61.461	
Application Reference Number	52-A0071/S01/S02 and ACT:SC/26-A0001	
System Name 2	Multi Venue Jackpot System – Local Controller (NSW Venue Wide Jackpot System)	
Manufacturer	Paltronics Australasia Pty Ltd	
Category	Subsidiary Equipment	
Specification Number	52.YC004	
System Description	64 Jackpot Levels Mystery Linked Progressive Jackpot System with CCCE Jackpot Transfer and Dual Port functionality with up to 200 Attached Gaming Machines.	
Technical Standards
Submission Standards	NS 10.3 + NSW Appendix (dated 24/04/13)
NSW CPTS 2.3; NSW JP TS Rev 1.3	
System Version	02.01.00.24	
SEI Interface Version	2.17 (Pala 5)	
Application Reference Number	52-A0071/S01/S02 and ACT:SC/26-A0001	
System Name 3	Multi-Venue Jackpot System – Mystery Madness Local Controller (NSW Venue Wide Jackpot System)	
Manufacturer	Paltronics Australasia Pty Ltd	
Category	Subsidiary Equipment	
Specification Number	52.YCM01	
System Description	4 Jackpot Level Local Mystery Madness Jackpot Controller with CCCE Jackpot Transfer and Dual Port functionality	
Technical Standards
Submission Standards	NS 10.3 + NSW Appendix (dated 24/04/13)
NSW CPTS 2.3; NSW JP TS Rev 1.3	
System Version	02.01.00.25	
SEI Interface Version	2.17 (Pala 5)	
Application Reference Number	52-A0071/S01/S02	
Specific Approval Conditions
1.	The logic cage(s) housing the logic boards and other sensitive components of the MVJS (the MVJS Server and each attached local jackpot controller) must be closed and key-locked at all times, except during system maintenance or upgrade of the MVJS
2.	The MVJS logic cages’ lock key(s) must be under the control of the venue manager.	

Continued
3.	The MVJS must be configured to use a different session encryption key every 24 hours or more frequently. The session encryption key is the “password” used by the MVJS to encrypt all its communications between the MVJS Server, Local Jackpot Controllers and Config/Console Workstations
4.	The ability to perform any server administration, system configuration, software modification and/or control the servers’ operation remotely must be disabled at all times, except during system maintenance or upgrade of the MVJS.
5.	Dedicated communication line (physical or logical) must be used for all communications between the MVJS Server, Local Jackpot Controllers and Config/Console Workstations.
6.	‘Rolled-up turnover’ is not approved for use in ACT and must be disabled at all times.
7.	‘Offline play’ is not approved for use in ACT and must be disabled at all times. The parameters “Maximum Offline Play Time” and “Maximum Offline Turnover” must be set to zero for each operating jackpot level.
8.	The supplier must limit the number of inter-venue gaming machines operating with an MVJS to 100 unless the testing outlined in the OLGR Application Testing Report is carried out prior to increasing the number of inter-venue gaming machines. Please note that licencees cannot increase the number of gaming machines operated with an MVJS unless they have sought an amendment to their Multi User Permit.